{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M9"]
[]
[]
[]
[]
["","","","","","2AMXM40M4V1B9","2AMXM50M4V1B9"]
["Размери","Тяло","","Височина","мм","552","552"]
["","","","Широчина","мм","852","852"]
["","","","Дълбочина","мм","350","350"]
["Тегло","Тяло","","","кг","36","41"]
["Електромотор на вентилатор","Скорост","Охлаждане","Свръх ниска","обор.","500","500"]
["","","Отопление","Свръх ниска","обор.","320","500"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°CDB","-10","-10"]
["","","","Макс.","°CDB","46","46"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","-15","-15"]
["","","","Макс.","°C с влажен термометър","18","18"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","46","48"]
["","Отопление","","Висок","dBA","48","50"]
["Хладилен агент","Тип","","","","R-32","R-32"]
["","Зареждане","","","кг","0.88","1.15"]
["","Маса","","","tCO2Eq","0.60","0.78"]
["","Потенциал на глобално затопляне","","","","675","675"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","20 (1)","20 (1)"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 20 м)","0,02 (за дължина на тръбопровод, надвишаваща 20 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","15","15"]
["","","Вътр. у-во - Вътр. у-во","Макс.","м","7.5","7.5"]
["","Обща дължина на тръбите","Система","Текуща","м","30","30"]
["Стандартни аксесоари","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Screw bag","","","","1","1"]
["Електрозахранване","Фаза","","","","1~","1~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","220-230-240","220-230-240"]
["Забележки","","","","","(1) - За една стая","(1) - За една стая"]
["Стандартни аксесоари","Reducer assembly","","","","","1"]