{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-A8"]
[]
[]
[]
[]
["","","","","","2MXM50A2V1B8","2MXM68A2V1B8"]
["Размери","Тяло","","Височина","мм","552","734"]
["","","","Широчина","мм","852","974"]
["","","","Дълбочина","мм","350","408"]
["Тегло","Тяло","","","кг","41","60"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°CDB","-10","-10"]
["","","","Макс.","°CDB","50","50"]
["Ниво на звуково налягане","Охлаждане","","Ном.","dBA","48","48"]
["","Отопление","","Ном.","dBA","50","48"]
["Хладилен агент","Тип","","","","R-32","R-32"]
["","Зареждане","","","кг","1.15","2.00"]
["","Маса","","","tCO2Eq","0.78","1.35"]
["","Потенциал на глобално затопляне","","","","675","675"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","20 (1)","25 (1)"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 20 м)","0,02 (за дължина на тръбопровод, надвишаваща 30 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","15","15"]
["","","Вътр. у-во - Вътр. у-во","Макс.","м","7.5","7.5"]
["","Обща дължина на тръбите","Система","Текуща","м","30","50"]
["Стандартни аксесоари","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Диапазон на енергийна ефективност","","","","","A+++ ~ D","A+++ ~ D"]
["Електрозахранване","Фаза","","","","1~","1~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","220-240","220-240"]
["Забележки","","","","","(1) - За една стая","(1) - За една стая"]
["","","","","","(2) - За комбинация с  CVXM-A, FVXM-A - максималната дължина на тръбите е 30 m.","(2) - За комбинация с  CVXM-A, FVXM-A - максималната дължина на тръбите е 30 m."]
["","","","","","(3) - Вж. отделния чертеж за работен диапазон","(3) - Вж. отделния чертеж за работен диапазон"]
["","","","","","(4) - Вж. отделния чертеж за електрическите схеми","(4) - Вж. отделния чертеж за електрическите схеми"]
["","","","","","(5) - Съдържа флуорирани парникови газове","(5) - Съдържа флуорирани парникови газове"]
["Стандартни аксесоари","Drain cap","","","","","3"]