{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Ниво на звуково налягане","Отопление","","Ном.","дБА","48","48","","50","50"]
["","Охлаждане","","Ном.","дБА","47","47","","48","48"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1","1","","1","1"]
["","Плик за винтове","","","","1","1","","1","1"]
["","Тапа за източващ отвор","","","","1","1","","1","1"]
["Хладилен агент","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","Потенциал на глобално затопляне","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Charge","","","kg","1.20","1.20","","1.60","1.60"]
["","Тип","","","","R-410A","R-410A","","R-410A","R-410A"]
["Тръбни връзки","Разлика в нивата","Вътр. у-во - Вътр. у-во","Макс.","м","7.5","7.5","","7.5","7.5"]
["","","Вътр. у-во - Външ. у-во","Макс.","м","15","15","","15","15"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 20 м)","0,02 (за дължина на тръбопровод, надвишаваща 20 м)","","0,02 (за дължина на тръбопровод, надвишаваща 20 м)","0,02 (за дължина на тръбопровод, надвишаваща 20 м)"]
["","Обща дължина на тръбите","Система","Текуща","м","30","30","","30","30"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Размери","Тяло","","Широчина","мм","765","765","","765","765"]
["","","","Дълбочина","мм","285","285","","285","285"]
["","","","Височина","мм","550","550","","550","550"]
["Тегло","Тяло","","","kg","38","38","","42","42"]
["Power supply","Фаза","","","","1~","1~","","1~","1~"]
["","Честота","","","Хц","50","50","","50","50"]
["","Напрежение","","","V","220-240","220-240","","220-240","220-240"]
["Забележки","","","","","(1) - Съдържа флуорирани парникови газове","(1) - Съдържа флуорирани парникови газове","","(1) - Съдържа флуорирани парникови газове","(1) - Съдържа флуорирани парникови газове"]
["Размери","Тяло","","Височина","мм","","","550","","","550"]
["","","","Широчина","мм","","","765","","","765"]
["","","","Дълбочина","мм","","","285","","","285"]
["Тегло","Тяло","","","kg","","","38","","","42"]
["Компресор","Тип","","","","","","Херметично запечатан люлеещ се компресор","","","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°C (сух термометър)","","","10","","","10"]
["","","","Макс.","°C (сух термометър)","","","46","","","46"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","","","-15","","","-15"]
["","","","Макс.","°C с влажен термометър","","","15.5","","","15.5"]
["Ниво на звуково налягане","Охлаждане","","Ном.","дБА","","","47","","","48"]
["","Отопление","","Ном.","дБА","","","48","","","50"]
["Хладилен агент","Тип","","","","","","R-410A","","","R-410A"]
["","Зареждане","","","kg","","","1.20","","","1.60"]
["","Маса","","","tCO2Eq","","","2.5","","","3.3"]
["","Потенциал на глобално затопляне","","","","","","2087.5","","","2087.5"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","","","20","","","20"]
["","Допълнително количество хладилен агент","","","кг/м","","","0,02 (за дължина на тръбопровод, надвишаваща 20 м)","","","0,02 (за дължина на тръбопровод, надвишаваща 20 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","","","15","","","15"]
["","","Вътр. у-во - Вътр. у-во","Макс.","м","","","7.5","","","7.5"]
["","Обща дължина на тръбите","Система","Текуща","м","","","30","","","30"]
["Стандартни аксесоари","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Електрозахранване","Фаза","","","","","","1~","","","1~"]
["","Честота","","","Хц","","","50","","","50"]
["","Напрежение","","","V","","","220-240","","","220-240"]
["Стандартни аксесоари","Редуциращ блок","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]