{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N7"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B7","3MXM52N2V1B7","3MXM68N2V1B7"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Свръх ниска","м³/мин","","","24.1"]
["","","Отопление","Свръх ниска","м³/мин","","","24.1"]
["","","","Свръх ниска","cfm","","","851"]
["","","Отопление","Свръх ниска","cfm","","","851"]
["Размери","Тяло","","Височина","мм","734","734","734"]
["","","","Широчина","мм","974","974","958"]
["","","","Дълбочина","мм","401","401","340"]
["Тегло","Тяло","","","кг","57","57","62"]
["Електромотор на вентилатор","Скорост","Охлаждане","Свръх ниска","обор.","420","420"]
["","","Отопление","Свръх ниска","обор.","420","420"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°CDB","-10","-10","-10"]
["","","","Макс.","°CDB","46","46","46"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","","","-15"]
["","","","Макс.","°C с влажен термометър","","","24"]
["Ниво на звуково налягане","Охлаждане","","Ном.","dBA","46","46","48"]
["","Отопление","","Ном.","dBA","47","47","48"]
["Хладилен агент","Тип","","","","R-32","R-32","R-32"]
["","Зареждане","","","кг","1.8","1.8","2"]
["","Маса","","","tCO2Eq","1.22","1.22"]
["","Потенциал на глобално затопляне","","","","675","675","675"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","25","25 (1)","25"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 30 м)","0,02 (за дължина на тръбопровод, надвишаваща 30 м)","0,02 (за дължина на тръбопровод, надвишаваща 30 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","15.0","15.0","15"]
["","","Вътр. у-во - Вътр. у-во","Макс.","м","7.5","7.5","7.5"]
["","Обща дължина на тръбите","Система","Текуща","м","50","50 (2)","50"]
["Стандартни аксесоари","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Електрозахранване","Фаза","","","","1~","1~","1~"]
["","Честота","","","Хц","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-440"]
["Забележки","","","","","(1) - За една стая","(1) - За една стая"]
["","","","","","(2) - За комбинация с  CVXM-A, FVXM-A - максималната дължина на тръбите е 30 m.","(2) - За комбинация с  CVXM-A, FVXM-A - максималната дължина на тръбите е 30 m."]
["Компресор","Тип","","","","","","Херметично запечатан люлеещ се компресор"]
["Стандартни аксесоари","Ръководство за монтаж","","","","","","1"]
["","Капачка за източващ отвор","","","","","","3"]
["","Тапа за източващ отвор","","","","","","1"]
["","Редуциращ блок","","","","","","1"]
["","Плик за винтове","","","","","","1"]
["Диапазон на енергийна ефективност","","","","","","","A+++ ~ D"]