{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-N"]
[]
[]
[]
[]
["","","","","","4MXM68N2V1B (Archived)","4MXM80N2V1B (Archived)"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Свръх ниска","м³/мин","24.1","24.1"]
["","","Отопление","Свръх ниска","м³/мин","24.1","24.1"]
["","","","Свръх ниска","cfm","851","851.0"]
["","","Отопление","Свръх ниска","cfm","851.0","851.0"]
["Размери","Тяло","","Височина","mm","734","734"]
["","","","Широчина","mm","958","958"]
["","","","Дълбочина","mm","340","340"]
["Тегло","Тяло","","","кг","63","67"]
["Компресор","Type","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°CDB","-10","-10"]
["","","","Макс.","°CDB","46","46"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","-15","-15"]
["","","","Макс.","°C с влажен термометър","18","18"]
["Ниво на звуково налягане","Охлаждане","","Ном.","дБА","48","49"]
["","Отопление","","Ном.","дБА","48","49"]
["Хладилен агент","Тип","","","","R-32","R-32"]
["","Зареждане","","","кг","2.00","2.40"]
["","Маса","","","tCO2Eq","1.4","1.6"]
["","Потенциал на глобално затопляне","","","","675","675"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","25","25"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 30 м)","0,02 (за дължина на тръбопровод, надвишаваща 30 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","15","15"]
["","","Вътр. у-во - Вътр. у-во","Макс.","м","7.5","7.5"]
["","Обща дължина на тръбите","Система","Текуща","м","60","70"]
["Стандартни аксесоари","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Електрозахранване","Фаза","","","","1~","1~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","220-240","220-240"]