{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5XXM-A"]
[]
[]
[]
[]
["","","","","","5XXM68A2V1B","5XXM90A2V1B"]
["Размери","Тяло","","Височина","мм","734","734"]
["","","","Широчина","мм","1040","1040"]
["","","","Дълбочина","мм","408","408"]
["Тегло","Тяло","","","кг","69.0","73.0"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°CDB","-10","-10"]
["","","","Макс.","°CDB","50","50"]
["Ниво на звуково налягане","Охлаждане","","Ном.","dBA","48.0 (2)","52.0 (2)"]
["","Отопление","","Ном.","dBA","49.0 (2), 51.0 (3)","53.0 (2), 55.0 (3)"]
["Хладилен агент","Тип","","","","R-32","R-32"]
["","Зареждане","","","кг","2.00","2.40"]
["","Маса","","","tCO2Eq","1.35","1.62"]
["","Потенциал на глобално затопляне","","","","675","675.0"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","25 (4) (5)","25 (5) (4)"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 30 м)","0,02 (за дължина на тръбопровод, надвишаваща 30 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","15.0 (5)","15.0 (5)"]
["","","Вътр. у-во - Вътр. у-во","Макс.","м","7.5 (5)","7.5 (5)"]
["","Обща дължина на тръбите","Система","Текуща","м","60","75"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1","1"]
["","Капачка за източващ отвор","","","","3","3"]
["","Тапа за източващ отвор","","","","1","1"]
["","Редуциращ блок","","","","1","1"]
["","Плик за винтове","","","","2","2"]
["Диапазон на енергийна ефективност","","","","","A+++ ~ D","A+++ ~ D"]
["Електрозахранване","Фаза","","","","1~","1~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","220-240","220-240"]
["Забележки","","","","","(1) - Вж. отделните чертежи за работен диапазон","(1) - Вж. отделните чертежи за работен диапазон"]
["","","","","","(2) - For DX combination","(2) - For DX combination"]
["","","","","","(3) - For Space heating operation of CHVX07 unit","(3) - For Space heating operation of CHVX07 unit"]
["","","","","","(4) - За една стая","(4) - За една стая"]
["","","","","","(5) - For combination with FBA71/100/125 refer to installation manual","(5) - For combination with FBA71/100/125 refer to installation manual"]
["","","","","","(6) - Съдържа флуорирани парникови газове","(6) - Съдържа флуорирани парникови газове"]