{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Стандартни аксесоари","Ръководство за монтаж","","","","Ръководство за монтаж"]
["","Ръководство за работа","","","","Ръководство за работа"]
["","Винт+Шайба","","","","Винт+Шайба"]
["","Безжично дистанционно управление","","","","Безжично дистанционно управление"]
["","Блокираща решетка на капака","","","","Блокираща решетка на капака"]
["","Батерия","","","","Батерия"]
["Тръбни съединения","Tечност","","Вън. д.","мм","9.52"]
["","Газ","","Вън. д.","мм","15.88"]
["","Дренаж","","","","19.05"]
["Входяща мощност","Охлаждане","","Ном.","кВт","0.128"]
["","Отопление","","Ном.","кВт","0.128"]
["Ниво на звукова мощност","Охлаждане","","","дБА","64"]
["","Отопление","","","дБА","64"]
["Размери","Тяло","","Широчина","мм","600"]
["","","","Дълбочина","мм","1,007"]
["","","","Височина","мм","285"]
["Корпус","Материал","","","","Галванизирана стомана"]
["Тегло","Тяло","","","kg","35"]
["Вентилатор","Външно статично налягане","","Високо","Pa","90"]
["","","","Ном.","Pa","77"]
["","","","Ниско","Pa","64"]
["Power supply","Фаза","","","","1~"]
["","Честота","","","Хц","50"]
["","Име","","","","V1"]
["","Напрежение","","","V","220-240"]
["Входяща мощност","Отопление","","Ном.","кВт","","0.109"]
["","Охлаждане","","Ном.","кВт","","0.109"]
["Вентилатор","Външно статично налягане","","Високо","Pa","","70","150","150"]
["","","","Ниско","Pa","","45","111","92"]
["Корпус","Материал","","","","","Галванизирана стомана"]
["Размери","Тяло","","Височина","мм","","378","378","378"]
["","","","Широчина","мм","","541","1300","1500"]
["","","","Дълбочина","мм","","1045","541","541"]
["Тегло","Тяло","","","kg","","44","50","56"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","","22.7","40.5","48.7"]
["","","","Ном.","м³/мин","","20.5","37","44"]
["","","","Ниско","м³/мин","","18.3","34.8","37.9"]
["","","Отопление","Висок","м³/мин","","22.7","40.5","48.7"]
["","","","Ном.","м³/мин","","20.5","37.4","43.9"]
["","","","Ниско","м³/мин","","18.3","34.8","37.9"]
["","Външно статично налягане","","Ном.","Pa","","57","128","122"]
["Звукова мощност","Охлаждане","","","дБА","","60","72","73"]
["","Отопление","","","дБА","","60","72","73"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","","41","53","55"]
["","","","Ном.","дБА","","38"]
["","","","Ниско","дБА","","36","50","50"]
["","Отопление","","Висок","дБА","","41","53","55"]
["","","","Ном.","дБА","","38"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","","36","50","50"]
["Тръбни съединения","Tечност","","Вън. д.","мм","","9.52","9.52","9.52"]
["","Газ","","Вън. д.","мм","","15.88","15.9","15.9"]
["","Дренаж","","","","","19.05"]
["Стандартни аксесоари","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Електрозахранване","Фаза","","","","","1~"]
["","Честота","","","Хц","","50"]
["","Напрежение","","","V","","220-240"]
["Капацитет на охлаждане","Общ капацитет","","Ном.","кВт","","","12.10","13.00"]
["Капацитет на отопление","Общ капацитет","","Ном.","кВт","","","13.5","15.5"]
["Корпус","Цвят","","","","","","Галванизирана стоманена пластина / небоядисана","Галванизирана стоманена пластина / небоядисана"]
["Вентилатор","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","","","37","44"]
["","","Отопление","Среден","м³/мин","","","37.4","43.9"]
["Ниво на звуково налягане","Охлаждане","","Среден","дБА","","","52","53"]
["","Отопление","","Среден","дБА","","","52","53"]
["Системи за управление","Инфрачервено дистанционно управление","","","","","","ARCWLA","ARCWLA"]