{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-C / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ACQ71CV1 / AZQS71B2V1B","ACQ100CV1 / AZQS100B8V1B","ACQ125CV1 / AZQS125B8V1B"]
["Капацитет на охлаждане","Ном.","","kW","6.8","9.5","12.1"]
["Охлаждане с конвекция","SEER","","","4.65","4.65"]
["","Годишно потребление на електроенергия","","kWh/a","512","716"]
["","Капацитет","Pdesign","kW","6.80","9.50"]
["","Клас на енергийна ефективност","","","B","B"]
["Отопление с конвекция (умерен климат)","Капацитет","Pdesign","kW","6.33","7.60"]
["","SCOP/A","","","3.80","3.80"]
["","Клас на енергийна ефективност","","","A","A"]
["","Годишно потребление на електроенергия","","kWh/a","2,332","2,800"]
["Номинална ефективност","Годишен разход на енергия","","kWh","1,025","1,480","2,010"]
["","EER","","","3.31","3.21","3.01"]
["","COP","","","3.61","3.61","3.41"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","B","A"]
["","","Отопление","","A","A"]
["Топлинен капацитет","Ном.","","kW","7.50","10.80","13.5"]
["Забележки","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]