{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Входяща мощност","Отопление","","Ном.","кВт","0.106","0.149"]
["","Охлаждане","","Ном.","кВт","0.106","0.149"]
["Вентилатор","Външно статично налягане","","Високо","Pa","0","0","0","0"]
["","","","Ниско","Pa","0","0","0","0"]
["Капацитет на охлаждане","Общ капацитет","","Ном.","кВт","","","12.10","13.00"]
["Капацитет на отопление","Общ капацитет","","Ном.","кВт","","","13.5","15.5"]
["Корпус","Цвят","","","","Бяло","Бяло","Бяло","Бяло"]
["","Материал","","","","Галванизирана стомана","Галванизирана стомана"]
["Размери","Тяло","","Височина","mm","260","260","260","285"]
["","","","Широчина","mm","1320","1538","1790","1900"]
["","","","Дълбочина","mm","634","634","634","680"]
["Тегло","Тяло","","","kg","38","45","65","70"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","23.8","31.1","34.4","43.9"]
["","","","Ном.","м³/мин","21.3","27.8","31","39"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","","","31","39"]
["","","","Ниско","м³/мин","18.9","24.8","27.2","28.3"]
["","","Отопление","Висок","м³/мин","23.8","31.1","34.4","43.9"]
["","","","Ном.","м³/мин","21.3","27.8","30.6","39.1"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","","","30.6","39.1"]
["","","Отопление","Ниско","м³/мин","18.9","24.8","27.2","28.3"]
["","Външно статично налягане","","Ном.","Pa","0","0","0","0"]
["Звукова мощност","Охлаждане","","","dBA","59","64","65","71"]
["","Отопление","","","dBA","62","64","65","71"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","49","52","52","56"]
["","","","Ном.","dBA","48","47"]
["","","","Среден","dBA","","","50","53"]
["","","","Ниско","dBA","46","46","49","46"]
["","Отопление","","Висок","dBA","49","52","52","56"]
["","","","Среден","dBA","","","50","53"]
["","","","Ном.","dBA","48","47"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","46","46","49","46"]
["Тръбни съединения","Tечност","","Вън. д.","mm","9.52","9.52","9.52","9.52"]
["","Газ","","Вън. д.","mm","15.88","15.88","15.9","15.9"]
["","Дренаж","","","","19.05","19.05"]
["Системи за управление","Инфрачервено дистанционно управление","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Жично дистанционно управление","","","","ARCWB","ARCWB"]
["Стандартни аксесоари","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Тръба за източване","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Електрозахранване","Фаза","","","","1~","1~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","220-240","220-240"]