{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXC-C"]
[]
[]
[]
[]
["","","","","","ARXC20CV1B","ARXC25CV1B","ARXC35CV1B","ARXC50CV1B","ARXC60CV1B","ARXC71CV1B"]
["Размери","Тяло","","Височина","мм","550","550","550","615","615","695"]
["","","","Широчина","мм","658","658","658","845","845","930"]
["","","","Дълбочина","мм","273","273","273","300","300","350"]
["Тегло","Тяло","","","кг","24","24","26","39","39","45"]
["Компресор","Тип","","","","Херметично въртене","Херметично въртене","Херметично въртене","Херметично въртене","Херметично въртене","Херметично въртене"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°CDB","10","10","10","-10","-10","-10"]
["","","","Макс.","°CDB","46","46","46","46","46","46"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","-15","-15","-15","-15","-15","-15"]
["","","","Макс.","°C с влажен термометър","18","18","18","18","18","18"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","45","45","46","51","54","54"]
["Хладилен агент","Тип","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Зареждане","","","кг","0.55","0.55","0.75","1","1.1","1.15"]
["","Маса","","","tCO2Eq","0.371","0.371","0.506","0.675","0.743","0.776"]
["","Потенциал на глобално затопляне","","","","675.0","675.0","675.0","675.0","675.0","675.0"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","20","20","20","30","30","30"]
["","Допълнително количество хладилен агент","","","кг/м","0, 017 (за дължина на тръбопровод, надвишаваща 7,5 m)","0, 017 (за дължина на тръбопровод, надвишаваща 7,5 m)","0, 017 (за дължина на тръбопровод, надвишаваща 7,5 m)","0, 017 (за дължина на тръбопровод, надвишаваща 7,5 m)","0, 017 (за дължина на тръбопровод, надвишаваща 7,5 m)","0, 017 (за дължина на тръбопровод, надвишаваща 7,5 m)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","15.0","15.0","15.0","20.0","20.0","20.0"]
["Електрозахранване","Фаза","","","","1~","1~","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]