{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":9,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXF-E"]
[]
[]
[]
[]
["","","","","","ARXF20E5V1B","ARXF25E5V1B","ARXF35E5V1B","ARXF42E5V1B"]
["Размери","Тяло","","Височина","мм","556","556","556","556"]
["","","","Широчина","мм","740","740","740","740"]
["","","","Дълбочина","мм","343","343","343","343"]
["Тегло","Тяло","","","кг","24.0","24.0","24.0","28.0"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°C със сух термометър","-10","-10","-10","-10"]
["","","","Макс.","°C със сух термометър","48","48","48","48"]
["","Отопление","околна температура","Мин.","°C (влажен термометър)","-15","-15","-15","-15"]
["","","","Макс.","°C (влажен термометър)","18","18","18","18"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","46.0","46.0","48.0","48.0"]
["","Отопление","","Висок","dBA","47.0","47.0","48.0","48.0"]
["Хладилен агент","Тип","","","","R-32","R-32","R-32","R-32"]
["","Зареждане","","","кг","0.420","0.420","0.550","0.750"]
["","Маса","","","tCO2Eq","0.280","0.280","0.370","0.510"]
["","Потенциал на глобално затопляне","","","","675.0","675.0","675.0","675.0"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","20","20","20","20"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","12.0","12.0","12.0","12.0"]
["Стандартни аксесоари","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Електрозахранване","Фаза","","","","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-240","220-240"]