{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Ниво на звуково налягане","Отопление","","Ном.","dBA","","49.0"]
["","Охлаждане","","Ном.","dBA","","49.0"]
["Стандартни аксесоари","Тапа за източващ отвор","","","","","1"]
["","Ръководство за монтаж","","","","","1"]
["","Етикет за маса на хладилен агент","","","","","1"]
["","Етикети на няколко езика за флуорираните парникови газове","","","","","1"]
["","Общи мерки за безопасност","","","","","1"]
["Хладилен агент","Charge","","","TCO2Eq","","0.52"]
["","Потенциал на глобално затопляне","","","","","675"]
["","Charge","","","kg","","0.76"]
["","Тип","","","","","R-32"]
["Работен диапазон","Охлаждане","околна температура","Макс.","°C със сух термометър","","50 (4), 46 (5)"]
["","","","Мин.","°C със сух термометър","","-10"]
["Тръбни съединения","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","","15"]
["","Допълнително количество хладилен агент","","","кг/м","","0,02 (за дължина на тръбопровод, надвишаваща 10 м)"]
["Компресор","Type","","","","","Херметично запечатан люлеещ се компресор"]
["Размери","Тяло","","Широчина","mm","","840"]
["","","","Дълбочина","mm","","350"]
["","","","Височина","mm","","552"]
["Тегло","Тяло","","","kg","","32"]
["Power supply","Phase","","","","","1~"]
["","Честота","","","Хц","","50"]
["","Напрежение","","","V","","220-240"]
["Забележки","","","","","(1) - Възможно само в комбинация с ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Съдържа флуорирани парникови газове"]
["","","","","","(2) - Възможно само в комбинация с ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Вж. отделния чертеж за работен диапазон"]
["","","","","","","(3) - Вж. отделния чертеж за електрическите схеми"]
["","","","","","","(4) - Възможно само в комбинация с ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Възможно само в комбинация с ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Размери","Тяло","","Височина","mm","552"]
["","","","Широчина","mm","840"]
["","","","Дълбочина","mm","350"]
["Тегло","Тяло","","","kg","32"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°C със сух термометър","-10"]
["","","","Макс.","°C със сух термометър","50 (4), 46 (5)"]
["Ниво на звуково налягане","Охлаждане","","Ном.","dBA","46.0"]
["","Отопление","","Ном.","dBA","47.0"]
["Хладилен агент","Зареждане","","","kg","0.76"]
["","Маса","","","tCO2Eq","0.52"]
["","Потенциал на глобално затопляне","","","","675"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","20"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 10 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","15"]
["Стандартни аксесоари","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Електрозахранване","Честота","","","Хц","50"]