{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS35L3V1B","ARXS25L3V1B (Archived)"]
["Ниво на звуково налягане","Отопление","","Висок","дБА","48"]
["","","","Ниско","дБА","45"]
["Стандартни аксесоари","1","","","","550"]
["Хладилен агент","Зареждане","","","kg","2.5"]
["","Тип","","","","1.2"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Свръх ниска","м³/мин","30.1"]
["","","","Свръх ниска","cfm","1,063"]
["Fan motor","Скорост","Охлаждане","Свръх ниска","обор.","740"]
["","","Отопление","Свръх ниска","обор.","-15"]
["Работен диапазон","Отопление","околна температура","Мин.","°C (влажен термометър)","20"]
["","","","Макс.","°C (влажен термометър)","10"]
["Ниво на звуково налягане","Охлаждане","","Ниско","дБА","44"]
["","","","Висок","дБА","48"]
["Компресор","Type","","","","Херметично запечатан люлеещ се компресор"]
["Размери","Тяло","","Широчина","mm","285"]
["","","","Дълбочина","mm","612"]
["","","","Височина","mm","765"]
["Тегло","Тяло","","","kg","34"]
["Вентилатор","Скорост на въздушния поток","Отопление","Свръх ниска","cfm","904"]
["","","","Свръх ниска","м³/мин","25.6"]
["Power supply","Фаза","","","","1~"]
["","Честота","","","Хц","50"]
["","Напрежение","","","V","220-240"]
["Забележки","","","","","(1) - Съдържа флуорирани парникови газове","(1) - 220V"]
["","","","","","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 230V","(3) - 240V"]
["","","","","","(4) - 240V"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Свръх ниска","м³/мин","","30.1"]
["","","Отопление","Свръх ниска","м³/мин","","25.6"]
["","","","Свръх ниска","cfm","","1063"]
["","","Отопление","Свръх ниска","cfm","","904"]
["Размери","Тяло","","Височина","mm","","550"]
["","","","Широчина","mm","","765"]
["","","","Дълбочина","mm","","285"]
["Тегло","Тяло","","","kg","","34"]
["Електромотор на вентилатор","Скорост","Охлаждане","Свръх ниска","обор.","","780"]
["","","Отопление","Свръх ниска","обор.","","740"]
["Компресор","Тип","","","","","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°C (сух термометър)","","10"]
["","","","Макс.","°C (сух термометър)","","46"]
["","Отопление","околна температура","Мин.","°C (влажен термометър)","","-15"]
["","","","Макс.","°C (влажен термометър)","","18"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","","46"]
["","Отопление","","Висок","дБА","","47"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","","44"]
["Хладилен агент","Тип","","","","","R-410A"]
["","Зареждане","","","kg","","1.0"]
["","Маса","","","tCO2Eq","","2.1"]
["","Потенциал на глобално затопляне","","","","","2087.5"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","","20"]
["","Допълнително количество хладилен агент","","","кг/м","","0,02 (за дължина на тръбопровод, надвишаваща 10 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","","15"]
["Стандартни аксесоари","Installation manual","","","","","1"]
["","Refrigerant charge label","","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1"]
["","Drain plug","","","","","1"]
["Електрозахранване","Фаза","","","","","1~"]
["","Честота","","","Хц","","50"]
["","Напрежение","","","V","","220-240"]