{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":11,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXC-B"]
[]
[]
[]
[]
["","","","","","ATXC20BV1B","ATXC25BV1B","ATXC35BV1B","ATXC50BV1B","ATXC60BV1B","ATXC71BV1B"]
["Входяща мощност","Охлаждане","","Ном.","кВт","0.6","0.775","1.06","1.57","1.915","2.41"]
["","Отопление","","Ном.","кВт","0.67","0.755","1.075","1.515","1.725","2.49"]
["Корпус","Цвят","","","","Бяло","Бяло","Бяло","Бяло","Бяло","Бяло"]
["","Материал","","","","Високоударен полистирол","Високоударен полистирол","Високоударен полистирол","Високоударен полистирол","Високоударен полистирол","Високоударен полистирол"]
["Размери","Тяло","","Височина","мм","288","288","288","288","297","297"]
["","","","Широчина","мм","785","785","785","785","1005","1005"]
["","","","Дълбочина","мм","250","250","250","250","288","288"]
["Тегло","Тяло","","","кг","9","9","9.5","9.5","13","13"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","10.8","10.8","10.8","12.2","20.4","20.4"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","8.8","8.8","9.1","10.2","15.9","15.9"]
["","","","Ниско","м³/мин","6.5","6.5","6.5","8.2","13.6","13.6"]
["","","","Тих режим","м³/мин","5.4","5.4","5.4","7.4","10.2","10.2"]
["Звукова мощност","Охлаждане","","","дБА","54","54","55","57","60","60"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","38","38","39","45","46","46"]
["","","","Среден","дБА","33","33","34","39","42","42"]
["","","","Ниско","дБА","26","26","26","33","38","38"]
["","","","Тих режим","дБА","20","20","21","29","30","30"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Газ","","Вън. д.","мм","9.52","9.52","9.52","12.7","12.7","12.7"]
["","Дренаж","","","","16.5","16.5","16.5","16.5","16.5","16.5"]
["Електрозахранване","Име","","","","V1","V1","V1","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]