{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B","ATXF25A5V1B (Archived)","ATXF35A5V1B (Archived)"]
["Ниво на звуково налягане","Отопление","","Висок","дБА","40","42","44","45"]
["","","","Среден","дБА","34","38","40","41"]
["","","","Тих режим","дБА","21","30","32","33"]
["","","","Ниско","дБА","28","33","35","36"]
["","Охлаждане","","Medium","дБА","33","39","41","42"]
["","","","Тих режим","дБА","20","31","33","34"]
["","","","Ниско","дБА","26","34","36","37"]
["","","","Висок","дБА","40","43","45","46"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1","1","1","1"]
["","Ръководство за работа","","","","1","1","1","1"]
["","Инфрачервено дистанционно","","","","1","1","1","1"]
["","Сухи батерии тип ААА","","","","2","2","2","2"]
["","Стойка за дистанционното","","","","1","1","1","1"]
["","Монтажна пластина:","","","","1","1","1","1"]
["","Фиксиращи винтове за вътрешното устройство","","","","2","2","2","2"]
["Системи за управление","Wired remote control","","","","BRC944B2, BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.35","6.35","6.35","6.35"]
["","Газ","","Вън. д.","мм","9.50","12.7","12.7","12.7"]
["","Дренаж","","","","18","18","18","18"]
["Входяща мощност","Охлаждане","","Ном.","кВт","0.019","0.029","0.032","0.032"]
["","Отопление","","Ном.","кВт","0.020","0.032","0.035","0.035"]
["Звукова мощност","Охлаждане","","","дБА","55","59","60","62"]
["","Отопление","","","дБА","55","61","62","62"]
["Размери","Тяло","","Широчина","мм","770","990","990","990"]
["","","","Дълбочина","мм","225","263","263","263"]
["","","","Височина","мм","286","295","295","295"]
["Корпус","Цвят","","","","Бяло","Бяло","Бяло","Бяло"]
["Тегло","Тяло","","","кг","8.50","13.5","13.5","13.5"]
["Вентилатор","Скорост на въздушния поток","Отопление","Висок","м³/мин","10.3","17.3","17.9","17.9"]
["","","","Ниско","м³/мин","6.7","12.2","12.8","12.8"]
["","","","Среден","м³/мин","8.6","14.8","15.8","15.8"]
["","","","Тих режим","м³/мин","5.3","10.7","11.3","11.3"]
["","","Охлаждане","Ниско","м³/мин","6.1","11.9","12.2","12.2"]
["","","","Среден","м³/мин","8.1","14.4","14.8","14.8"]
["","","","Висок","м³/мин","10.1","16.8","17.3","17.3"]
["","","","Тих режим","м³/мин","4.4","10.5","10.7","10.7"]
["Power supply","Фаза","","","","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50"]
["","Име","","","","","V1","V1","V1"]
["","Напрежение","","","V","220-240","220-240","220-240","220-240"]
["Входяща мощност","Охлаждане","","Ном.","кВт","","","","","0.019","0.032"]
["","Отопление","","Ном.","кВт","","","","","0.02","0.032"]
["Корпус","Цвят","","","","","","","","Бяло","Бяло"]
["Размери","Тяло","","Височина","мм","","","","","286","286"]
["","","","Широчина","мм","","","","","770","770"]
["","","","Дълбочина","мм","","","","","225","225"]
["Тегло","Тяло","","","кг","","","","","8.5","9"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","","","","","10.1","11.5"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","","","","","8.1","8.3"]
["","","","Ниско","м³/мин","","","","","6.1","6.3"]
["","","","Тих режим","м³/мин","","","","","4.4","4.5"]
["","","Отопление","Висок","м³/мин","","","","","10.3","11.5"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","","","","","8.6","9"]
["","","Отопление","Ниско","м³/мин","","","","","6.7","7"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","","","","","5.3","5.3"]
["Звукова мощност","Охлаждане","","","дБА","","","","","55","58"]
["","Отопление","","","дБА","","","","","55","58"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","","","","","40","43"]
["","","","Среден","дБА","","","","","33","34"]
["","","","Ниско","дБА","","","","","26","27"]
["","","","Тих режим","дБА","","","","","20","20"]
["","Отопление","","Висок","дБА","","","","","40","40"]
["","","","Среден","дБА","","","","","34","35"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","","","","","28","29"]
["","","","Тих режим","дБА","","","","","21","21"]
["Тръбни съединения","Tечност","","Вън. д.","мм","","","","","6.35","6.35"]
["","Газ","","Вън. д.","мм","","","","","9.5","9.5"]
["","Дренаж","","","","","","","","18","18"]
["Системи за управление","Инфрачервено дистанционно управление","","","","","","","","ARC470A1","ARC470A1"]
["","Жично дистанционно управление","","","","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Стандартни аксесоари","Installation manual","","","","","","","","1","1"]
["","AAA dry-cell batteries","","","","","","","","2","2"]
["","Operation manual","","","","","","","","1","1"]
["","Indoor unit fixing screws","","","","","","","","2","2"]
["","Infrared remote control","","","","","","","","1","1"]
["","Mounting plate","","","","","","","","1","1"]
["","Remote control holder","","","","","","","","1","1"]
["Електрозахранване","Фаза","","","","","","","","1~","1~"]
["","Честота","","","Хц","","","","","50","50"]
["","Напрежение","","","V","","","","","220-240","220-240"]