{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F"]
[]
[]
[]
[]
["","","","","","ATXF50F5V1B"]
["Входяща мощност","Охлаждане","","Ном.","кВт","0.04"]
["","Отопление","","Ном.","кВт","0.04"]
["Корпус","Цвят","","","","Бяло"]
["Размери","Тяло","","Височина","мм","286"]
["","","","Широчина","мм","770"]
["","","","Дълбочина","мм","225"]
["Тегло","Тяло","","","кг","9"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","12.6"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","9"]
["","","","Ниско","м³/мин","7.2"]
["","","","Тих режим","м³/мин","6.4"]
["","","Отопление","Висок","м³/мин","12.8"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","9.6"]
["","","Отопление","Ниско","м³/мин","7.2"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","6.4"]
["Звукова мощност","Охлаждане","","","дБА","59"]
["","Отопление","","","дБА","59"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","45"]
["","","","Среден","дБА","39"]
["","","","Ниско","дБА","34"]
["","","","Тих режим","дБА","31"]
["","Отопление","","Висок","дБА","44"]
["","","","Среден","дБА","38"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","33"]
["","","","Тих режим","дБА","30"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6"]
["","Газ","","Вън. д.","мм","12.7"]
["","Дренаж","","","","18"]
["Системи за управление","Инфрачервено дистанционно управление","","","","ARC480A93"]
["","Жично дистанционно управление","","","","BRC073A1"]
["Стандартни аксесоари","ATXF50F5V1B","","","","1"]
["","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Електрозахранване","Фаза","","","","1~"]
["","Честота","","","Хц","50"]
["","Напрежение","","","V","220-440"]
["Забележки","","","","","(1) - Охлаждане: температура на открито 27°C (сух термометър), 19°C (влажен термометър); външна температура 35°C със сух термометър; дължина на еквивал. тръбопр.: 5 м, денивелация: 0 м."]
["","","","","","(2) - Отопление: температура на открито 20°С (сух термометър), външна темп. 7°C (сух термометър), 6°C (влажен термометър); съответна дължина на тръбите за хладилния агент: 5 м (хоризонтално)"]
["","","","","","(3) - Вж. отделния чертеж за електрическите схеми"]