{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-G / 3AMXF-A9"]
[]
[]
[]
[]
["","","","","ATXF25G5V1B / ATXF25G5V1B / ATXF25G5V1B / 3AMXF52A2V1B9"]
["Капацитет на охлаждане","Мин.","","кВт","1.8"]
["","Ном.","","кВт","5.2"]
["","Макс.","","кВт","7"]
["Топлинен капацитет","Мин.","","кВт","1.3"]
["","Ном.","","кВт","6.8"]
["","Макс.","","кВт","8"]
["Номинална ефективност","EER","","","4.05"]
["","COP","","","3.88"]
["","Годишен разход на енергия","","kWh","642"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A"]
["","","Отопление","","A"]
["Охлаждане с конвекция","Клас на енергийна ефективност","","","A++"]
["","Капацитет","Pdesign","кВт","5.2"]
["","SEER","","","7.2"]
["","Годишно потребление на електроенергия","","kWh/a","253"]
["Отопление с конвекция (умерен климат)","Клас на енергийна ефективност","","","A+"]
["","Капацитет","Pdesign","кВт","5"]
["","SCOP/A","","","4.01"]
["","Pdh Капацитет на отопление при -10°","","кВт","3.74"]
["","Годишно потребление на електроенергия","","kWh/a","1744"]
["Диапазон на енергийна ефективност","","","","A+++ ~ D"]