{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-K3"]
[]
[]
[]
[]
["","","","","","ATXP20K3V1B","ATXP25K3V1B","ATXP35K3V1B"]
["Входяща мощност","Охлаждане","","Ном.","kW","0.017","0.019","0.032"]
["","Отопление","","Ном.","kW","0.02","0.02","0.032"]
["Корпус","Цвят","","","","Бяло","Бяло","Бяло"]
["Размери","Тяло","","Височина","мм","286","286","286"]
["","","","Широчина","мм","770","770","770"]
["","","","Дълбочина","мм","225","225","225"]
["Тегло","Тяло","","","kg","9","9","9"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","9.8","10.1","11.5"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","7.9","8.1","8.3"]
["","","","Ниско","м³/мин","5.9","6.1","6.3"]
["","","","Тих режим","м³/мин","4.4","4.4","4.5"]
["","","Отопление","Висок","м³/мин","10.3","10.3","11.5"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","8.4","8.6","9"]
["","","Отопление","Ниско","м³/мин","6.5","6.7","7"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","5.3","5.3","5.3"]
["Звукова мощност","Охлаждане","","","дБА","55","55","58"]
["","Отопление","","","дБА","55","55","58"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","39","40","43"]
["","","","Среден","дБА","33","33","34"]
["","","","Ниско","дБА","25","26","27"]
["","","","Тих режим","дБА","20","20","20"]
["","Отопление","","Висок","дБА","39","40","40"]
["","","","Среден","дБА","34","34","35"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","28","28","29"]
["","","","Тих режим","дБА","21","21","21"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.35","6.35","6.35"]
["","Газ","","Вън. д.","мм","9.5","9.5","9.5"]
["","Дренаж","","","","18","18","18"]
["Системи за управление","Infrared remote control","","","","ARC480A11","ARC480A11"]
["Системи за управление","Жично дистанционно управление","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Стандартни аксесоари","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Електрозахранване","Фаза","","","","1~","1~","1~"]
["","Честота","","","Хц","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-240"]
["Системи за управление","Инфрачервено дистанционно управление","","","","","","ARC480A11"]