{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXS-K / ARXS-L3"]
[]
[]
[]
[]
["","","","","ATXS25K2V1B / ARXS25L3V1B","ATXS25K3V1B / ARXS25L3V1B","ATXS35K2V1B / ARXS35L3V1B","ATXS35K3V1B / ARXS35L3V1B"]
["Капацитет на охлаждане","Мин.","","кВт","","","","1.4"]
["","Макс.","","кВт","","","","4.0"]
["","Ном.","","кВт","2.5","2.5 (2)","3.5","3.5 (2)"]
["Тръбни съединения","Tечност","Вън. д.","мм","","6.35","","6.35"]
["","Газ","Вън. д.","мм","","9.5","","9.5"]
["","Дренаж","вън. д.","мм","","18","","18"]
["Номинална ефективност","Годишен разход на енергия","","kWh","301","301","473","473"]
["","EER","","","4.15","4.15 (1)","3.70","3.70 (1)"]
["","COP","","","4.52","4.52 (1)","4.76","4.76 (1)"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A","A","A","A"]
["","","Отопление","","A","A","A","A"]
["Капацитет на отопление","Ном.","","кВт","2.8","2.8 (2)","4.00","4.00 (2)"]
["","Мин.","","кВт","","1.3","","1.4"]
["","Макс.","","кВт","","4.7","","5.2"]
["Забележки","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]
["","","","","","(3) - 220V","","(3) - 220V"]
["","","","","","(4) - 230V","","(4) - 230V"]
["","","","","","(5) - 240V","","(5) - 240V"]