{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AVA-A"]
[]
[]
[]
[]
["","","","","","AVA125AMVE"]
["Капацитет на охлаждане","Общ капацитет","","Ном.","kW","12.10"]
["Капацитет на отопление","Общ капацитет","","Ном.","kW","13.5"]
["Корпус","Цвят","","","","Свежо бяло"]
["Размери","Тяло","","Височина","mm","1850"]
["","","","Широчина","mm","600"]
["","","","Дълбочина","mm","350"]
["Тегло","Тяло","","","кг","50"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","28"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","26"]
["","","","Ниско","м³/мин","24"]
["","","Отопление","Висок","м³/мин","28"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","26"]
["","","Отопление","Ниско","м³/мин","24"]
["Звукова мощност","Охлаждане","","","дБА","63"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","51"]
["","","","Среден","дБА","48"]
["","","","Ниско","дБА","46"]
["","Отопление","","Висок","дБА","51"]
["","","","Среден","дБА","46"]
["","","","Ном.","дБА","48"]
["Тръбни съединения","Tечност","","Вън. д.","mm","9.52"]
["","Газ","","Вън. д.","mm","15.9"]
["","Дренаж","","","","I.D. 20/O.D. 26"]
["Системи за управление","Жично дистанционно управление","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Стандартни аксесоари","Installation manual","","","","1"]
["","Hole protection rubber","","","","2"]
["","Cover","","","","1"]
["","Dew proof material","","","","1"]
["","Remote control wiring","","","","1"]
["","Bracket for installation","","","","1"]
["","Operation manual","","","","1"]
["","Bush","","","","1"]
["","Installation pattern","","","","1"]
["","Insulation for fitting for gas pipe","","","","1"]
["","Insulation for fitting for liquid pipe","","","","1"]
["","Screws","","","","5"]
["","Tie-wraps","","","","5"]
["Електрозахранване","Фаза","","","","1~"]
["","Честота","","","Хц","50/60"]
["","Напрежение","","","V","220-240/220"]