{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BAEF125AWB"]
[]
[]
[]
[]
["","","","","BAEF125AWB."]
["Входяща мощност","кВт","","","0.006"]
["Корпус","Цвят","","","Gray"]
["","Работен светодиод","Цвят","","Blue/red"]
["Размери","Тяло","Височина","мм","100"]
["","","Широчина","мм","840"]
["","","Дълбочина","мм","840"]
["","Комплектовано тяло","Височина","мм","168"]
["","","Широчина","мм","910"]
["","","Дълбочина","мм","910"]
["Тегло","Тяло","","kg","12.0"]
["","Комплектовано тяло","","kg","15.5"]
["Компл.","Материал","","","Картово табло"]
["","тегло","","kg","4"]
["Power supply","Фаза","","","1~"]
["","Честота","","Хц","50/60"]
["","Напрежение","","V","220-240/220"]
["Забележки","","","","(1) - С 2 сензора (регулаторен коефициент 0,65): A+ ; Други: A"]