{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000676"]
[]
[]
[]
[]
["","","","","","BR00000676."]
["Приложение","","","","","Подов тип"]
["Капацитет","м³/мин","","","","33.33"]
["Корпус","Цвят","","","","Покритие от боядисана галванизирана стомана"]
["Размери","Тяло","","Височина","мм","1628"]
["","","","Широчина","мм","720"]
["","","","Дълбочина","мм","770"]
["Тегло","Тяло","","","kg","150"]
["Приложим размер на стая","m²","","","","133"]
["Операция за пречистване на въздуха","Входяща мощност","","Височина","kW","0.379"]
["Ниво на звуково налягане","Операция за пречистване на въздуха","","Висок","дБА","55.9"]
["Вентилатор","Скорост на въздушния поток","Операция за пречистване на въздуха","Турбо","m³/h","2300"]
["","","","Висок","m³/h","2000"]
["Предпазни устройства","Артикул","","01","","Предпазен изключвател (работата спира, когато задният панел се отвори)"]
["Стандартни аксесоари","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Захранващ кабел-=-м","м","","","","3"]
["Електрозахранване","Честота","","","Хц","50/60"]
["Течащ ток","Операция за пречистване на въздуха","","Висок","A","1.73"]