{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDK"]
[]
[]
[]
[]
["","","","","BRC1HHDAK (Archived)","BRC1HHDAKA (Archived)"]
["Корпус","Цвят","","","Черно","Черно"]
["","Покритие на бутон","","","Не","Не"]
["","Работен светодиод","Цвят","","Син индикатор за състояние","Син индикатор за състояние"]
["Размери","Тяло","Височина","мм","85","85"]
["","","Широчина","мм","85","85"]
["","","Дълбочина","мм","25","25"]
["","Комплектовано тяло","Височина","мм","50","50"]
["","","Широчина","мм","217","217"]
["","","Дълбочина","мм","161","161"]
["Тегло","Тяло","","kg","0.110","0.110"]
["","Комплектовано тяло","","kg","0.317","0.317"]
["Компл.","Материал","","","Картово табло","Картово табло"]
["","тегло","","kg","0.0850","0.0850"]
["LCD","Тип","","","100 x 150 пикс.","100 x 150 пикс."]
["","Размери","Височина","мм","40.7","40.7"]
["","","Широчина","мм","28.0","28.0"]
["","Фонова светлина","Цвят","","Бяло","Бяло"]
["Температура на околната среда","Работа","Мин.","°C","-10","-10"]
["","","Макс.","°C","50","50"]
["","Съхранение","Мин.","°C","-20","-20"]
["","","Макс.","°C","70","70"]
["","Температура на околната среда-=-Относителна влажност <-=-%","","%","95","95"]
["Системи за управление","Клас на термоконтрол","","","VI","VI"]
["","Системи за управление-=-Участие в сезонната ефективност на отопление с конвекция-=-%","","%","4.0","4.0"]
["Връзки на окабеляване","Дължина на проводниците","Макс.","м","500","500"]