{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 3MXM-N7"]
[]
[]
[]
[]
["","","","","","CHYHBH05AFV32 / 3MXM52N2V1B7"]
["Загряване на битова гореща вода","Общо","","Обявен график на натоварване","","XL"]
["","Умерен климат","","Клас на енергийна ефективност на загряване на вода","","A"]
["COP","","","","","4.49 (1)"]
["Отопление с конвекция","Изходяща вода при средни климат. условия 55°C","Общо","Клас на сезонна ефективност при отопление","","A+"]
["","","","ηs (Сезонна ефективност на отопление)","%","111.4"]
["","","","SCOP","","2.86"]
["Топлинен капацитет","Ном.","","","kW","4.41 (1)"]
["Забележки","","","","","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), заобиколен котел"]