{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BB"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BB"]
["Ниво на звуково налягане","Отопление","","Висок","dBA","39"]
["","","","Среден","dBA","32"]
["","","","Тих режим","dBA","21"]
["","","","Ниско","dBA","25"]
["","Охлаждане","","Среден","dBA","32"]
["","","","Тих режим","dBA","21"]
["","","","Ниско","dBA","25"]
["","","","Висок","dBA","39"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1"]
["","Ръководство за работа","","","","1"]
["","Въздушен филтър","","","","2"]
["","Инфрачервено дистанционно","","","","1"]
["","Монтажна пластина за дистанционно","","","","1"]
["","Плик за винтове","","","","1"]
["","Винтов капак","","","","2"]
["","Сухи батерии тип ААА","","","","2"]
["","Общи мерки за безопасност","","","","1"]
["Хладилен агент","Потенциал на глобално затопляне","","","","675.0"]
["Системи за управление","Жично дистанционно управление","","","","BRC073"]
["","Инфрачервено дистанционно управление","","","","ARC466A58"]
["Тръбни съединения","Tечност","","Вън. д.","mm","6.35"]
["","Газ","","Вън. д.","mm","9.50"]
["","Дренаж","","","","18"]
["Консумирана мощност","Охлаждане","","Ном.","kW","0.020"]
["","Отопление","","Ном.","kW","0.020"]
["Sound power level","Охлаждане","","","dBA","57"]
["Размери","Тяло","","Широчина","mm","798"]
["","","","Дълбочина","mm","189"]
["","","","Височина","mm","295"]
["Корпус","Цвят","","","","Черно"]
["Тегло","Тяло","","","кг","11.5"]
["Вентилатор","Скорост на въздушния поток","Отопление","Висок","м³/мин","10.9"]
["","","","Среден","м³/мин","8.7"]
["","","","Ниско","м³/мин","6.4"]
["","","","Тих режим","м³/мин","4.5"]
["","","Охлаждане","Ниско","м³/мин","6.1"]
["","","","Среден","м³/мин","8.2"]
["","","","Висок","м³/мин","11.0"]
["","","","Тих режим","м³/мин","4.6"]
["Power supply","Фаза","","","","1~"]
["","Име","","","","V1"]
["","Честота","","","Хц","50"]
["","Напрежение","","","V","220-240"]