{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R / 3MXM-A9"]
[]
[]
[]
[]
["","","","","CTXM15R2V1B / CTXM15R2V1B / CTXM15R2V1B / 3MXM40A2V1B9","CTXM15R5V1B / CTXM15R5V1B / CTXM15R5V1B / 3MXM40A2V1B9"]
["Капацитет на охлаждане","Ном.","","кВт","4.00","4.00"]
["Топлинен капацитет","Ном.","","кВт","4.60","4.60"]
["Номинална ефективност","EER","","","5.18","5.18"]
["","COP","","","5.17","5.17"]
["","Годишен разход на енергия","","kWh","386","386"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A","A"]
["","","Отопление","","A","A"]
["Охлаждане с конвекция","Клас на енергийна ефективност","","","A+++","A+++"]
["","Капацитет","Pdesign","кВт","4.00","4.00"]
["","SEER","","","8.55","8.55"]
["","Годишно потребление на електроенергия","","kWh/a","164","164"]
["Отопление с конвекция (умерен климат)","Клас на енергийна ефективност","","","A++","A++"]
["","Капацитет","Pdesign","кВт","4.90","4.90"]
["","SCOP/A","","","4.65","4.65"]
["","Pdh Капацитет на отопление при -10°","","кВт","4.00","4.00"]
["","Годишно потребление на електроенергия","","kWh/a","1475","1475"]