{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B","CTXM15R5V1B"]
["Входяща мощност","Охлаждане","","Ном.","kW","0.029","0.029"]
["","Отопление","","Ном.","kW","0.023","0.023"]
["Корпус","Цвят","","","","Бяло","Бяло"]
["Размери","Тяло","","Височина","мм","295","295"]
["","","","Широчина","мм","778","778"]
["","","","Дълбочина","мм","272","272"]
["Тегло","Тяло","","","kg","10","10"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","10.5","10.5"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","7.5","7.5"]
["","","","Ниско","м³/мин","5.7","5.7"]
["","","","Тих режим","м³/мин","4.3","4.3"]
["","","Отопление","Висок","м³/мин","9.3","9.3"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","8.2","8.2"]
["","","Отопление","Ниско","м³/мин","6.2","6.2"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","5.1","5.1"]
["Звукова мощност","Охлаждане","","","дБА","57","57"]
["","Отопление","","","дБА","54","54"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","41","41"]
["","","","Среден","дБА","33","33"]
["","","","Ниско","дБА","25","25"]
["","","","Тих режим","дБА","19","19"]
["","Отопление","","Висок","дБА","39","39"]
["","","","Среден","дБА","34","34"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","26","26"]
["","","","Тих режим","дБА","20","20"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.35","6.35"]
["","Газ","","Вън. д.","мм","9.5","9.5"]
["","Дренаж","","","","18","18"]
["Системи за управление","Infrared remote control","","","","ARC466A67","ARC466A67"]
["Системи за управление","Жично дистанционно управление","","","","BRC073A1","BRC073A1"]
["Стандартни аксесоари","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Електрозахранване","Име","","","","V1","V1"]
["","Фаза","","","","1~","1~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","220-240","220-240"]