{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":7,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B (Archived)","CTXM15R5V1B (Archived)"]
["Входяща мощност","Охлаждане","","Ном.","кВт","0.029","0.029"]
["","Отопление","","Ном.","кВт","0.023","0.023"]
["Корпус","Цвят","","","","Бяло","Бяло"]
["Размери","Тяло","","Височина","мм","295","295"]
["","","","Широчина","мм","778","778"]
["","","","Дълбочина","мм","272","272"]
["Тегло","Тяло","","","кг","10","10"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","10.5","10.5"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","7.5","7.5"]
["","","","Ниско","м³/мин","5.7","5.7"]
["","","","Тих режим","м³/мин","4.3","4.3"]
["","","Отопление","Висок","м³/мин","9.3","9.3"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","8.2","8.2"]
["","","Отопление","Ниско","м³/мин","6.2","6.2"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","5.1","5.1"]
["Звукова мощност","Охлаждане","","","dBA","57","57"]
["","Отопление","","","dBA","54","54"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","41","41"]
["","","","Среден","dBA","33","33"]
["","","","Ниско","dBA","25","25"]
["","","","Тих режим","dBA","19","19"]
["","Отопление","","Висок","dBA","39","39"]
["","","","Среден","dBA","34","34"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","26","26"]
["","","","Тих режим","dBA","20","20"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.35","6.35"]
["","Газ","","Вън. д.","мм","9.5","9.5"]
["","Дренаж","","","","18","18"]
["Системи за управление","Инфрачервено дистанционно управление","","","","ARC466A67","ARC466A67"]
["","Жично дистанционно управление","","","","BRC073A1","BRC073A1"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1","1"]
["","Безжично дистанционно управление","","","","1","1"]
["","Сухи батерии тип ААА","","","","2","2"]
["","Адаптерен комплект за WLAN","","","","1","1"]
["","Ръководство за работа","","","","1","1"]
["","Обезмирисяващ филтър с титанов апатит","","","","1","1"]
["","Фиксиращи винтове за вътрешното устройство","","","","2","2"]
["","Монтажна пластина:","","","","1","1"]
["","Стойка за дистанционното","","","","1","1"]
["Диапазон на енергийна ефективност","","","","","A+++ ~ D","A+++ ~ D"]
["Електрозахранване","Име","","","","V1","V1"]
["","Фаза","","","","1~","1~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","220-240","220-240"]
["Забележки","","","","","(1) - Охлаждане: температура на открито 27°C със сух термометър, 19.0°C с влажен термометър; външна темп. 35°C със сух термометър; 24°C с влажен термометър; съответстваща дължина на тръбопр.: 5м","(1) - Охлаждане: температура на открито 27°C със сух термометър, 19.0°C с влажен термометър; външна темп. 35°C със сух термометър; 24°C с влажен термометър; съответстваща дължина на тръбопр.: 5м"]
["","","","","","(2) - Отопление: температура на открито 20°С (сух термометър), външна темп. 7°C (сух термометър), 6°C (влажен термометър); съответна дължина на тръбите за хладилния агент: 5м","(2) - Отопление: температура на открито 20°С (сух термометър), външна темп. 7°C (сух термометър), 6°C (влажен термометър); съответна дължина на тръбите за хладилния агент: 5м"]