{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Ниво на звуково налягане","Отопление","","Висок","дБА","38","","41"]
["","","","Тих режим","дБА","21","","21"]
["","","","Ниско","дБА","28","","30"]
["","Охлаждане","","Тих режим","дБА","21","","21"]
["","","","Ниско","дБА","25","","28"]
["","","","Висок","дБА","37","","42"]
["","","","Ном.","дБА","33"]
["","Охлаждане","","Ном.","дБА","31","","35"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1","","1"]
["","Ръководство за работа","","","","1","","1"]
["","Безжично дистанционно управление","","","","1","","1"]
["","Батерии","","","","2","","2"]
["","Стойка за дистанционното","","","","1","","1"]
["","Монтажна пластина:","","","","1","","1"]
["","Фиксиращи винтове за вътрешното устройство","","","","2","","2"]
["","Филтър за фотокаталитично пречистване на въздуха от титанов апатит","","","","2","","2"]
["Системи за управление","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Тръбни съединения","Tечност","","Вън. д.","mm","6.35","","6.35"]
["","Газ","","Вън. д.","mm","9.5","","9.5"]
["","Дренаж","","","","18","","18"]
["Входяща мощност","Охлаждане","","Ном.","kW","0.040","","0.040"]
["","Отопление","","Ном.","kW","0.040","","0.040"]
["Звукова мощност","Охлаждане","","","дБА","55","","59"]
["","Отопление","","","дБА","56","","58"]
["Размери","Тяло","","Широчина","mm","780","","780"]
["","","","Дълбочина","mm","215","","215"]
["","","","Височина","mm","289","","289"]
["Корпус","Colour","","","","Бяло","","Бяло"]
["Тегло","Тяло","","","кг","8","","8"]
["Вентилатор","Скорост на въздушния поток","Отопление","Висок","м³/мин","","","10.1"]
["","","","Ниско","м³/мин","","","6.3"]
["","","","Тих режим","м³/мин","","","4.3"]
["","","Охлаждане","Ниско","м³/мин","","","5.2"]
["","","","Висок","м³/мин","","","9.2"]
["","","","Тих режим","м³/мин","","","3.9"]
["","","","Ном.","м³/мин","","","8.1"]
["","","Охлаждане","Ном.","м³/мин","","","7.2"]
["Power supply","Фаза","","","","1~","","1~"]
["","Честота","","","Хц","50","","50"]
["","Име","","","","V1","","V1"]
["","Напрежение","","","V","220-240","","220-240"]
["Забележки","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Входяща мощност","Охлаждане","","Ном.","kW","","0.04","","0.040"]
["","Отопление","","Ном.","kW","","0.04","","0.040"]
["Корпус","Цвят","","","","","Бяло","","Бяло"]
["Размери","Тяло","","Височина","mm","","289","","289"]
["","","","Широчина","mm","","780","","780"]
["","","","Дълбочина","mm","","215","","215"]
["Тегло","Тяло","","","кг","","8","","8.00"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","","7.9","","9.2"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","","6.3","","7.2"]
["","","","Ниско","м³/мин","","4.7","","5.2"]
["","","","Тих режим","м³/мин","","3.9","","3.9"]
["","","Отопление","Висок","м³/мин","","9","","10.1"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","","7.5","","8.1"]
["","","Отопление","Ниско","м³/мин","","6","","6.3"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","","4.3","","4.3"]
["Звукова мощност","Охлаждане","","","дБА","","55","","59"]
["","Отопление","","","дБА","","56","","58"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","","37","","42"]
["","","","Среден","дБА","","31","","35"]
["","","","Ниско","дБА","","25","","28"]
["","","","Тих режим","дБА","","21","","21"]
["","Отопление","","Висок","дБА","","38","","41"]
["","","","Среден","дБА","","33","","36"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","","28","","30"]
["","","","Тих режим","дБА","","21","","21"]
["Тръбни съединения","Tечност","","Вън. д.","mm","","6.35","","6.35"]
["","Газ","","Вън. д.","mm","","9.5","","9.50"]
["","Дренаж","","","","","18","","18"]
["Системи за управление","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Стандартни аксесоари","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Електрозахранване","Име","","","","","V1","","V1"]
["","Фаза","","","","","1~","","1~"]
["","Честота","","","Хц","","50","","50"]
["","Напрежение","","","V","","220-240","","220-240"]