{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Входяща мощност","кВт","","","","0.015"]
["Максимален брой вътрешни тела, които могат да се свързват","","","","","32"]
["Максимален брой външни тела, които могат да се свързват @","","","","","7"]
["Размери","Тяло","","Височина","мм","136"]
["","","","Широчина","мм","384"]
["","","","Дълбочина","мм","92"]
["Комуникация","DIII-NET","","Количество","","1"]
["","","","Забележка","","DIII-NET (F1F2)"]
["","Ethernet","","Количество","","1"]
["","Вход. клема","Цифрова","Количество","","4"]
["Температура на околната среда","Работа","","Мин.","°C","-10"]
["","","","Макс.","°C","50"]
["","Съхранение","","Мин.","°C","-20"]
["","","","Макс.","°C","60"]
["","Температура на околната среда-=-Относителна влажност <-=-%","","","%","85"]
["Електрозахранване","Честота","","","Хц","50/60"]
["","Напрежение","","","V","110-240 AC"]
["Забележки","","","","","(1) - Включва консумираната мощност на електрозахранващия блок WAGO, модула на процесора и входно-изходния модул"]
["","","","","","(2) - Размерите включват електрозахранващия блок WAGO, модула на процесора, входно-изходния модул и необходимото отстояние между различните части"]
["","","","","","(3) - Размерите на допълнителния екран са: височина: 209 mm, ширина: 123 mm, дълбочина: 8,5 mm"]