{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":7,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBBH-D6V / ERLA-DW17"]
[]
[]
[]
[]
["","","","","","EBBH16DF6V / ERLA16DAW17","EBBH16DF6V / ERLA16D2W17"]
["Топлинен капацитет","Ном.","","","кВт","16.0 (2) (1)","16.0 (1) (2)"]
["Входяща мощност","Отопление","","Ном.","кВт","3.53 (1), 4.56 (2)","3.53 (1), 4.56 (2)"]
["COP","","","","","4.53 (1), 3.51 (2)","4.53 (1), 3.51 (2)"]
["Отопление с конвекция","Изходяща вода при средни климат. условия 55°C","Общо","SCOP","","3.32","3.32"]
["","","","Клас на сезонна ефективност при отопление","","A++","A++"]
["","Изходяща вода при средни климат. условия 35°C","Общо","SCOP","","4.61","4.61"]
["","","","Клас на сезонна ефективност при отопление","","A+++","A+++"]
["Забележки","","","","","(1) - Условие: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Условие: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Условие: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(4) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]
["","","","","","(5) - Измерено при спад на налягане от 10 kPa в системата за отопление при работно състояние на изходящата вода от 47-55°C в стая с температура 20°C. DB/WB 7°C/6°.","(5) - Измерено при спад на налягане от 10 kPa в системата за отопление при работно състояние на изходящата вода от 47-55°C в стая с температура 20°C. DB/WB 7°C/6°."]