{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSH-D / ERLA-DV37"]
[]
[]
[]
[]
["","","","","","EBSH16P30DF / ERLA16D2V37","EBSH16P50DF / ERLA16D2V37","EBSH16P30DF / ERLA16DAV37","EBSH16P50DF / ERLA16DAV37"]
["Вътрешно тяло","","","","","EBSH16P30DF","EBSH16P50DF","EBSH16P30DF","EBSH16P50DF"]
["Топлинен капацитет","Ном.","","","кВт","16.0 (1)","16.0 (1)","16.0 (1)","16.0 (1)"]
["Входяща мощност","Отопление","","Ном.","кВт","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)"]
["COP","","","","","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)"]
["Загряване на битова гореща вода ","Общо","","Обявен график на натоварване","","L","XL","L","XL"]
["Загряване на битова гореща вода","Умерен климат","","Клас на енергийна ефективност на загряване на вода","","A+","A+","A+","A+"]
["Отопление с конвекция","Изходяща вода при средни климат. условия 55°C","Общо","SCOP","","3.32","3.32","3.32","3.32"]
["","","","Клас на сезонна ефективност при отопление","","A++","A++","A++","A++"]
["","Изходяща вода при средни климат. условия 35°C","Общо","SCOP","","4.61","4.61","4.61","4.61"]
["","","","Клас на сезонна ефективност при отопление","","A+++","A+++","A+++","A+++"]
["Забележки","","","","","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]