{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":13,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSXB-D / ERLA11-14DV3"]
[]
[]
[]
[]
["","","","","","EBSXB11P30DF / ERLA11D2V3","EBSXB11P50DF / ERLA11D2V3","EBSXB11P30DF / ERLA11DAV3","EBSXB11P50DF / ERLA11DAV3","EBSXB16P30DF / ERLA14D2V3","EBSXB16P50DF / ERLA14D2V3","EBSXB16P30DF / ERLA14DAV3","EBSXB16P50DF / ERLA14DAV3"]
["Indoor unit","","","","","EBSXB11P30DF","EBSXB11P50DF","EBSXB11P30DF","EBSXB11P50DF","EBSXB16P30DF","EBSXB16P50DF","EBSXB16P30DF","EBSXB16P50DF"]
["Топлинен капацитет","Ном.","","","кВт","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)"]
["Капацитет на охлаждане","Ном.","","","кВт","11.2 (2)","11.2 (2)","11.2 (2)","11.2 (2)","12.9 (2)","12.9 (2)","12.9 (2)","12.9 (2)"]
["Входяща мощност","Отопление","","Ном.","кВт","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)"]
["","Охлаждане","","Ном.","кВт","3.47 (2)","3.47 (2)","3.47 (2)","3.47 (2)","4.34 (2)","4.34 (2)","4.34 (2)","4.34 (2)"]
["COP","","","","","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)"]
["EER","","","","","3.22 (2)","3.22 (2)","3.22 (2)","3.22 (2)","2.98 (2)","2.98 (2)","2.98 (2)","2.98 (2)"]
["Загряване на битова гореща вода ","Общо","","Обявен график на натоварване","","L","XL","L","XL","L","XL","L","XL"]
["Загряване на битова гореща вода","Умерен климат","","Клас на енергийна ефективност на загряване на вода","","A+","A+","A+","A+","A+","A+","A+","A+"]
["Отопление с конвекция","Изходяща вода при средни климат. условия 55°C","Общо","SCOP","","3.27","3.27","3.27","3.27","3.26","3.26","3.26","3.26"]
["","","","Клас на сезонна ефективност при отопление","","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Изходяща вода при средни климат. условия 35°C","Общо","SCOP","","4.72","4.72","4.72","4.72","4.68","4.68","4.68","4.68"]
["","","","Клас на сезонна ефективност при отопление","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Забележки","","","","","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]