{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-CB / ERHQ-BW17"]
[]
[]
[]
[]
["","","","","EHBH16CB3V / ERHQ014BAW17","EHBH16CB9W / ERHQ014BAW17"]
["COP","","","","4.24 (1), 3.22 (2)","4.24 (1), 3.22 (2)"]
["Топлинен капацитет","Ном.","","kW","14.5 (1), 13.6 (2)","14.5 (1), 13.6 (2)"]
["Входяща мощност","Отопление","Ном.","kW","3.42 (1), 4.21 (2)","3.42 (1), 4.21 (2)"]
["Забележки","","","","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]
["","","","","(3) - околна темп. 35°C - LWE 7°C (DT=5°C)","(3) - околна темп. 35°C - LWE 7°C (DT=5°C)"]
["","","","","(4) - Tamb 35°C - LWE 18°C (DT=5°C)","(4) - Tamb 35°C - LWE 18°C (DT=5°C)"]
["","","","","(5) - Сух термометър/влажен термометър 7°C/6°C-LWC 35°C(DT=5°C)","(5) - Сух термометър/влажен термометър 7°C/6°C-LWC 35°C(DT=5°C)"]
["","","","","(6) - DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)","(6) - DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)"]