{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-E / ERGA-EV7"]
[]
[]
[]
[]
["","","","","","EHSH04P30EF / ERGA04EAV37","EHSH04P30EG / ERGA04EAV37"]
["Indoor unit","","","","","EHSH04P30EF","EHSH04P30EG"]
["Топлинен капацитет","Ном.","","","kW","4.36 (1), 4.60 (2)","4.36 (1), 4.60 (2)"]
["Входяща мощност","Отопление","","Ном.","kW","0.830 (1), 1.26 (2)","0.830 (1), 1.26 (2)"]
["COP","","","","","5.23 (1), 3.65 (2)","5.23 (1), 3.65 (2)"]
["Загряване на битова гореща вода ","Общо","","Обявен график на натоварване","","L","L"]
["Загряване на битова гореща вода","Умерен климат","","Клас на енергийна ефективност на загряване на вода","","A+","A+"]
["Отопление с конвекция","Изходяща вода при средни климат. условия 55°C","Общо","SCOP","","3.26","3.26"]
["","","","Клас на сезонна ефективност при отопление","","A++","A++"]
["","Изходяща вода при средни климат. условия 35°C","Общо","SCOP","","4.88","4.88"]
["","","","Клас на сезонна ефективност при отопление","","A+++","A+++"]
["Забележки","","","","","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]
["Диапазон на енергийна ефективност","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]