{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-D3"]
[]
[]
[]
[]
["","","","","","EHSX04P50DA3","EHSX04P30DA3","EHSX08P30DA3","EHSX08P50DA3"]
["Корпус","Цвят","","","","Чисто бяло (RAL9016) / Тъмно сиво (RAL7011)","Чисто бяло (RAL9016) / Тъмно сиво (RAL7011)","Чисто бяло (RAL9016) / Тъмно сиво (RAL7011)","Чисто бяло (RAL9016) / Тъмно сиво (RAL7011)"]
["","Материал","","","","Удароустойчив пропилен","Удароустойчив пропилен","Удароустойчив пропилен","Удароустойчив пропилен"]
["Размери","Тяло","","Височина","мм","1896","1891","1891","1896"]
["","","","Широчина","мм","790","595","595","790"]
["","","","Дълбочина","мм","790","615","615","790"]
["Тегло","Тяло","","","kg","93.0","73.0","73.0","93.0"]
["PED (директива за оборудване под налягане)","Категория","","","","чл. 3.3","чл. 3.3","чл. 3.3","чл. 3.3"]
["Хладилен агент","Тип","","","","R-32","R-32","R-32","R-32"]
["","Потенциал на глобално затопляне","","","","675.0","675.0","675.0","675.0"]
["","Зареждане","","","kg","1.50","1.50","1.50","1.50"]
["Звукова мощност","Ном.","","","dBA","39","39","39","39"]
["Работен диапазон","Отопление","Водна страна","Мин.","°C","18","18","18","18"]
["","","","Макс.","°C","65","65","65","65"]
["","Охлаждане","околна температура","Мин.","°C (сух термометър)","10","10","10","10"]
["","","Водна страна","Мин.","°C","5","5","5","5"]
["","","","Макс.","°C","22","22","22","22"]
["Електрозахранване","Фаза","","","","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50"]
["","Напрежение","","","V","230","230","230","230"]
["Електрически нагревател","Електрозахранване","","Име","","3V / 9W","3V / 9W","3V / 9W","3V / 9W"]
["","","","Фаза","","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Честота","Хц","50","50","50","50"]
["Забележки","","","","","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃"]
["","","","","","(5) - Подгряване на водосъдържателя само с термопомпа, без електрически нагревател","","","(5) - Подгряване на водосъдържателя само с термопомпа, без електрически нагревател"]