{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-E"]
[]
[]
[]
[]
["","","","","","EHSX04P30EF","EHSX04P50EF","EHSX04P30EG","EHSX04P50EG","EHSX08P30EF","EHSX08P50EF","EHSX08P30EG","EHSX08P50EG"]
["Корпус","Цвят","","","","Чисто бяло (RAL9016) / Чисто черно (RAL9017)","Чисто бяло (RAL9016) / Чисто черно (RAL9017)","Чисто бяло (RAL9016) / Чисто черно (RAL9017)","Чисто бяло (RAL9016) / Чисто черно (RAL9017)","Чисто бяло (RAL9016) / Чисто черно (RAL9017)","Чисто бяло (RAL9016) / Чисто черно (RAL9017)","Чисто бяло (RAL9016) / Чисто черно (RAL9017)","Чисто бяло (RAL9016) / Чисто черно (RAL9017)"]
["","Материал","","","","Удароустойчив пропилен","Удароустойчив пропилен","Удароустойчив пропилен","Удароустойчив пропилен","Удароустойчив пропилен","Удароустойчив пропилен","Удароустойчив пропилен","Удароустойчив пропилен"]
["Размери","Тяло","","Височина","mm","1,892","1,905","1,891","1,910","1,892","1,905","1,891","1,910"]
["","","","Широчина","mm","594","792","594","792","594","792","594","792"]
["","","","Дълбочина","mm","644","812","644","817","644","812","644","817"]
["Тегло","Тяло","","","кг","77","107","77.0","97.0","77","107","77.0","97.0"]
["PED (директива за оборудване под налягане)","Категория","","","","Чл. 4.3","Чл. 4.3","Чл. 4.3","Чл. 4.3","Чл. 4.3","Чл. 4.3","Чл. 4.3","Чл. 4.3"]
["Хладилен агент","Тип","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Потенциал на глобално затопляне","","","","675","675","675.0","675.0","675","675","675.0","675.0"]
["","Зареждане","","","кг","1.5","1.5","1.50","1.50","1.5","1.5","1.50","1.50"]
["Звукова мощност","Ном.","","","дБА","39","39","39","39","39","39","39","39"]
["Работен диапазон","Отопление","Водна страна","Мин.","°C","18","18","18","18","18","18","18","18"]
["","","","Макс.","°C","65","65","65","65","65","65","65","65"]
["","Охлаждане","околна температура","Мин.","°C със сух термометър","10","10","10","10","10","10","10","10"]
["","","Водна страна","Мин.","°C","5","5","5","5","5","5","5","5"]
["","","","Макс.","°C","22","22","22","22","22","22","22","22"]
["Електрозахранване","Фаза","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50","50","50","50","50"]
["","Напрежение","","","V","230","230","230","230","230","230","230","230"]
["Забележки","","","","","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897"]