{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-CB / ERHQ-BV3"]
[]
[]
[]
[]
["","","","","EHVH11S18CB3V / ERHQ011BAV3","EHVH11S26CB9W / ERHQ011BAV3","EHVH16S18CB3V / ERHQ014BAV3","EHVH16S26CB9W / ERHQ014BAV3","EHVH16S18CB3V / ERHQ016BAV3","EHVH16S26CB9W / ERHQ016BAV3"]
["Загряване на битова гореща вода","Общо","Обявен график на натоварване","","L","XL","L","XL","L","XL"]
["","Умерен климат","Клас на енергийна ефективност на загряване на вода","","A","A","A","A","A","A"]
["COP","","","","4.39 (1), 3.25 (2)","4.39 (1), 3.25 (2)","4.29 (1), 3.24 (2)","4.29 (1), 3.24 (2)","4.08 (1), 3.20 (2)","4.08 (1), 3.20 (2)"]
["Топлинен капацитет","Ном.","","kW","11.2 (1), 10.3 (2)","11.2 (1), 10.3 (2)","14.0 (1), 13.1 (2)","14.0 (1), 13.1 (2)","16.0 (1), 15.2 (2)","16.0 (1), 15.2 (2)"]
["Power input","Отопление","Ном.","kW","2.55 (1), 3.17 (2)","2.55 (1), 3.17 (2)","3.26 (1), 4.04 (2)","3.26 (1), 4.04 (2)","3.92 (1), 4.75 (2)","3.92 (1), 4.75 (2)"]
["Забележки","","","","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]
["","","","","(3) - околна темп. 35°C - LWE 7°C (DT=5°C)","(3) - околна темп. 35°C - LWE 7°C (DT=5°C)","(3) - околна темп. 35°C - LWE 7°C (DT=5°C)","(3) - околна темп. 35°C - LWE 7°C (DT=5°C)","(3) - околна темп. 35°C - LWE 7°C (DT=5°C)","(3) - околна темп. 35°C - LWE 7°C (DT=5°C)"]
["","","","","(4) - Tamb 35°C - LWE 18°C (DT=5°C)","(4) - Tamb 35°C - LWE 18°C (DT=5°C)","(4) - Tamb 35°C - LWE 18°C (DT=5°C)","(4) - Tamb 35°C - LWE 18°C (DT=5°C)","(4) - Tamb 35°C - LWE 18°C (DT=5°C)","(4) - Tamb 35°C - LWE 18°C (DT=5°C)"]
["","","","","(5) - Сух термометър/влажен термометър 7°C/6°C-LWC 35°C(DT=5°C)","(5) - Сух термометър/влажен термометър 7°C/6°C-LWC 35°C(DT=5°C)","(5) - Сух термометър/влажен термометър 7°C/6°C-LWC 35°C(DT=5°C)","(5) - Сух термометър/влажен термометър 7°C/6°C-LWC 35°C(DT=5°C)","(5) - Сух термометър/влажен термометър 7°C/6°C-LWC 35°C(DT=5°C)","(5) - Сух термометър/влажен термометър 7°C/6°C-LWC 35°C(DT=5°C)"]
["","","","","(6) - DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)","(6) - DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)","(6) - DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)","(6) - DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)","(6) - DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)","(6) - DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)"]