{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":13,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-E9W / ERGA04-08EVA"]
[]
[]
[]
[]
["","","","","","EHVH08S18EA9W / ERGA06EAV3A","EHVH08S23EA9W / ERGA06EAV3A","EHVH08S18EJ9W / ERGA06EAV3A","EHVH08S23EJ9W / ERGA06EAV3A","EHVH08S18EA9W / ERGA08EAV3A","EHVH08S18EJ9W / ERGA08EAV3A","EHVH08S23EA9W / ERGA08EAV3A","EHVH08S23EJ9W / ERGA08EAV3A"]
["Топлинен капацитет","Ном.","","","kW","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Входяща мощност","Отопление","","Ном.","kW","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["Консумирана мощност","Битова гореща вода от 10°C до 50°C","","Ном.","kWh","2.48","3.01","2.48","3.01","2.48","2.48","3.01","3.01"]
["Време за загряване от 10°C до 50°C","hr","","","","1 ч. 28 мин.","1 ч. 40 мин.","1 ч. 28 мин.","1 ч. 40 мин.","1 ч. 28 мин.","1 ч. 28 мин.","1 ч. 40 мин.","1 ч. 40 мин."]
["COP","","","","","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Загряване на битова гореща вода ","Общо","","Обявен график на натоварване","","L","XL","L","XL","L","L","XL","XL"]
["Загряване на битова гореща вода","Умерен климат","","Клас на енергийна ефективност на загряване на вода","","A+","A+","A+","A+","A+","A+","A+","A+"]
["Отопление с конвекция","Изходяща вода при средни климат. условия 55°C","Общо","SCOP","","3.25","3.25","3.25","3.25","3.27","3.27","3.27","3.27"]
["","","","Клас на сезонна ефективност при отопление","","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Изходяща вода при средни климат. условия 35°C","Общо","SCOP","","4.47","4.47","4.47","4.47","4.56","4.56","4.56","4.56"]
["","","","Клас на сезонна ефективност при отопление","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Диапазон на енергийна ефективност","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Забележки","","","","","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]