{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E3V / ERGA04-08EVA"]
[]
[]
[]
[]
["","","","","","EHVX04S18EA3V / ERGA04EAV3A","EHVX04S18EJ3V / ERGA04EAV3A","EHVX04S23EA3V / ERGA04EAV3A","EHVX04S23EJ3V / ERGA04EAV3A"]
["Топлинен капацитет","Ном.","","","kW","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)"]
["Капацитет на охлаждане","Ном.","","","kW","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)"]
["Входяща мощност","Отопление","","Ном.","kW","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)"]
["","Охлаждане","","Ном.","kW","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)"]
["Консумирана мощност","Битова гореща вода от 10°C до 50°C","","Ном.","kWh","2.48","2.48","3.01","3.01"]
["Време за загряване от 10°C до 50°C","hr","","","","1 ч. 28 мин.","1 ч. 28 мин.","1 ч. 40 мин.","1 ч. 40 мин."]
["COP","","","","","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)"]
["EER","","","","","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)"]
["Загряване на битова гореща вода ","Общо","","Обявен график на натоварване","","L","L","XL","XL"]
["Загряване на битова гореща вода","Умерен климат","","Клас на енергийна ефективност на загряване на вода","","A+","A+","A+","A+"]
["Отопление с конвекция","Изходяща вода при средни климат. условия 55°C","Общо","SCOP","","3.29","3.29","3.29","3.29"]
["","","","Клас на сезонна ефективност при отопление","","A++","A++","A++","A++"]
["","Изходяща вода при средни климат. условия 35°C","Общо","SCOP","","4.54","4.54","4.54","4.54"]
["","","","Клас на сезонна ефективност при отопление","","A+++","A+++","A+++","A+++"]
["Диапазон на енергийна ефективност","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Забележки","","","","","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]