{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3 / EVLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AAV3 / EVLQ08CAV3","EHYHBX08AFV3 / EVLQ08CAV3"]
["Загряване на битова гореща вода","Общо","","Обявен график на натоварване","","XL"]
["","Умерен климат","","Клас на енергийна ефективност на загряване на вода","","A"]
["COP","","","","","4.45 (3), 3.42 (4)","4.45, 3.42"]
["Отопление с конвекция","Изходяща вода при средни климат. условия 55°C","Общо","Клас на сезонна ефективност при отопление","","A++"]
["","","","ηs (Сезонна ефективност на отопление)","%","129"]
["","","","SCOP","","3.29"]
["Капацитет на охлаждане","Ном.","","","кВт","6.86 (4), 5.36 (4)"]
["","Мин.","","","кВт","2.50 (3), 2.50 (4)"]
["EER","","","","","3.42 (3), 2.29 (4)","3.42, 2.29"]
["Топлинен капацитет","Ном.","","","кВт","7.40 (3), 6.89 (4)"]
["","Мин.","","","кВт","1.80 (3), 1.80 (4)"]
["","Макс.","","","кВт","10.0 (3), 9.53 (4)"]
["Входяща мощност","Охлаждане","","Ном.","кВт","2.01 (3), 2.34 (4)"]
["","Отопление","","Ном.","кВт","1.66 (3), 2.01 (4)"]
["Забележки","","","","","(1) - Условие: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Условие: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]
["","","","","","(3) - Условие 1 : Охлаждане Ta 35°C - LWE 18℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Tвънш. 35°C - LWE 7°C (Dt=5°C), заобиколен котел"]
["","","","","","(4) - Условие 2 : Охлаждане Ta 35°C - LWE 7℃ (DT = 5°C); отопление Ta DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(4) - Tвънш. 35°C - LWE 18℃ (Dt=5°C), заобиколен котел"]
["","","","","","(5) - Tвънш. 35°C - LWE 7°C (Dt=5°C), заобиколен котел","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), заобиколен котел"]
["","","","","","(6) - Tвънш. 35°C - LWE 18℃ (Dt=5°C), заобиколен котел","(6) - DB/WB 7°C/6°C - LWC 45℃ (DT=5°C), заобиколен котел"]
["","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), заобиколен котел"]
["","","","","","(8) - DB/WB 7°C/6°C - LWC 45℃ (DT=5°C), заобиколен котел"]
["Топлинен капацитет","Мин.","","","кВт","","1.80, 1.80"]
["","Ном.","","","кВт","","7.40, 6.89"]
["","Макс.","","","кВт","","10.0, 9.53"]
["Капацитет на охлаждане","Мин.","","","кВт","","2.50, 2.50"]
["","Ном.","","","кВт","","6.86, 5.36"]
["Входяща мощност","Отопление","","Ном.","кВт","","1.66, 2.01"]
["","Охлаждане","","Ном.","кВт","","2.01, 2.34"]
["Загряване на битова гореща вода ","Общо","","Обявен график на натоварване","","","XL"]
["Загряване на битова гореща вода","Умерен климат","","Клас на енергийна ефективност на загряване на вода","","","A"]
["Отопление с конвекция","Изходяща вода при средни климат. условия 55°C","Общо","SCOP","","","3.29"]
["","","","Клас на сезонна ефективност при отопление","","","A++"]
["","Изходяща вода при средни климат. условия 35°C","Общо","SCOP","","","4.28"]
["","","","Клас на сезонна ефективност при отопление","","","A++"]
["Диапазон на енергийна ефективност","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]