{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYKOMB-AA3"]
[]
[]
[]
[]
["","","","","","EHYKOMB33AA3"]
["Засмукване","Връзка","","Диаметър","мм","15"]
["Газ","Потребление (G20)","","Мин.","m³/h","0.79"]
["","","","Макс.","m³/h","3.39"]
["","Потребление (G25)","","Мин.","m³/h","0.89"]
["","","","Макс.","m³/h","3.92"]
["","Потребление (G31)","","Мин.","m³/h","0.30"]
["","","","Макс.","m³/h","1.29"]
["","Клас по NOx","","","","6"]
["","Ниво на NOx (G20)","","","mg/kWh","36"]
["Централно отопление","Подадена топлина в Qn (нетна калорийна стойност)","Ном.","Мин.","kW","7.6"]
["","","","Макс.","kW","27.0"]
["","Подадена топлина в Qn (брутна калорийна стойност)","Ном.","Мин.","kW","8.4"]
["","","","Макс.","kW","30.0"]
["","Изходяща Pn при 80/60°C","","Мин.","kW","7.5"]
["","","","Ном.","kW","26.6"]
["","Мощност при 37/30°C","","Ном.","kW","8.2"]
["","Температура на водата","","Макс.","°C","90"]
["Битова гореща вода","Подадена топлина (нетна калорийна стойност) в Qnw","Ном.","Мин.","kW","7.6"]
["","","","Макс.","kW","32.7"]
["","Подадена топлина (брутна калорийна стойност) в Qnw","Ном.","Мин.","kW","8.4"]
["","","","Макс.","kW","36.3"]
["","Клас на комфорт","","","","XL"]
["Битова гореща вода (EN13203)","Температура","","Макс.","°C","65"]
["Подаван въздух","Концентрично","","","","Не"]
["Димни газове","Температура","","Макс.","°C","70"]
["","Връзка","","","мм","60"]
["","Масов разход (G20)","","Макс.","кг/ч.","54.4"]
["","Масов разход (G25)","","Макс.","кг/ч.","54.4"]
["","Масов разход (G31)","","Макс.","кг/ч.","53.6"]
["Корпус","Цвят","","","","RAL9010"]
["","Материал","","","","Метален лист с покритие"]
["Размери","Тяло","Височина","Корпус","мм","710"]
["","","","Широчина","мм","450"]
["","","","Дълбочина","мм","240"]
["тегло","Тяло","","Празно","кг","36"]
["Загряване на битова гореща вода ","Общо","","Обявен график на натоварване","","XL"]
["Загряване на битова гореща вода","Общо","","Клас на енергийна ефективност на загряване на вода","","A"]
["Отопление с конвекция","Общо","","Клас сезонна ефективност на отопление с конвекция","","A"]