{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWET-BV3"]
[]
[]
[]
[]
["","","","","","EKHWET90BAV3","EKHWET120BAV3"]
["Mонтаж","","","","","Стена","Стена"]
["Корпус","Цвят","","","","Бяло + черно","Бяло + черно"]
["","Материал","","","","Ламарина, Акрилонитрилов бутадиенов стирол","Ламарина, Акрилонитрилов бутадиенов стирол"]
["Размери","Тяло","Височина","Водосъдържател","мм","1032","1283"]
["","","","Широчина","мм","510","510"]
["","","","Дълбочина","мм","570","570"]
["тегло","Тяло","","Празно","кг","43","47"]
["резервоар","Воден обем","","","l","89","118"]
["","Материал","","","","Емайлирана стомана съгл. DIN4753TL2","Емайлирана стомана съгл. DIN4753TL2"]
["Водосъдържател","Максимална температура на водата","","","°C","75.0","75.0"]
["","Клас на енергийна ефективност","","","","B","C"]
["Топлообменник","Домакинска гореща вода","","Количество","","1","1"]
["","","","Тръбен материал","","Алуминиев","Алуминиев"]
["","","","Работно налягане","бар","42","42"]
["Допълнителен нагревател","Капацитет","","","kW","1.2","1.2"]