{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH"]
[]
[]
[]
[]
["","","","","","ERGA06EAV3H"]
["Размери","Тяло","","Височина","мм","740"]
["","","","Широчина","мм","884"]
["","","","Дълбочина","мм","388"]
["Тегло","Тяло","","","кг","58.5"]
["Работен диапазон","Охлаждане","","Мин.","°CDB","10"]
["","","","Макс.","°CDB","43"]
["","Домакинска гореща вода","","Мин.","°CDB","-25"]
["","Битова гореща вода","","Макс.","°CDB","35"]
["Звукова мощност","Отопление","","Ном.","дБА","60 (1)"]
["","Охлаждане","","Ном.","дБА","62 (1)"]
["Ниво на звуково налягане","Отопление","","Ном.","дБА","47 (1)"]
["","Охлаждане","","Ном.","дБА","49 (1)"]
["Хладилен агент","Тип","","","","R-32"]
["","Потенциал на глобално затопляне","","","","675.0"]
["","Маса","","","tCO2Eq","1.01"]
["","Зареждане","","","кг","1.50"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6"]
["","Газ","","Вън. д.","мм","15.9"]
["","Дренаж","","вън. д.","мм","18"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","30.0"]
["","Топлоизолация","","","","Тръбите за газ и течност"]
["Електрозахранване","Име","","","","V3"]
["","Фаза","","","","1N~"]
["","Честота","","","Хц","50"]
["","Напрежение","","","V","230"]
["Ток","Препоръчани предпазители","","","A","20"]
["Забележки","","","","","(1) - Охлаждане Ta 35°C - LWE 18℃ (DT = 5℃); ОтоплениеTa DB/WB 7°C/6°C - LWC 35℃ (DT = 5°C)"]