{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DW17"]
[]
[]
[]
[]
["","","","","","ERLA16D2W17","ERLA16DAW17"]
["Размери","Тяло","","Височина","мм","870","870"]
["","","","Широчина","мм","1,100","1,100"]
["","","","Дълбочина","мм","460","460"]
["Тегло","Тяло","","","кг","101","101"]
["Вентилатор","Скорост на въздушния поток","Отопление","Висок","м³/мин","85.0","85.0"]
["","","Охлаждане","Висок","м³/мин","85","85"]
["Работен диапазон","Охлаждане","","Мин.","°CDB","10","10"]
["","","","Макс.","°CDB","43","43"]
["","Домакинска гореща вода","","Мин.","°CDB","-25","-25"]
["","Битова гореща вода","","Макс.","°CDB","25 (1), 35 (1)","25 (1), 35 (1)"]
["Звукова мощност","Отопление","","Ном.","дБА","62.0 (2)","62.0 (2)"]
["Ниво на звуково налягане","Отопление","","Ном.","дБА","48.0 (2)","48.0 (2)"]
["Хладилен агент","Тип","","","","R-32","R-32"]
["","Потенциал на глобално затопляне","","","","675.0","675.0"]
["","Маса","","","tCO2Eq","2.57","2.57"]
["","Зареждане","","","кг","3.8","3.8"]
["Тръбни съединения","Tечност","","Вън. д.","мм","9.5","9.5"]
["","Газ","","Вън. д.","мм","15.9","15.9"]
["","Дренаж","","вън. д.","мм","26","26"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","30.0","30.0"]
["","Топлоизолация","","","","Тръбите за газ и течност","Тръбите за газ и течност"]
["Електрозахранване","Име","","","","W1","W1"]
["","Фаза","","","","3~","3~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","400","400"]
["Ток","Препоръчани предпазители","","","A","16","16"]
["Забележки","","","","","(1) - За повече подробности, вижте диаграмата на работния диапазон","(1) - За повече подробности, вижте диаграмата на работния диапазон"]
["","","","","","(2) - Измерено при спад на налягане от 10 kPa в системата за отопление при работно състояние на изходящата вода от 47-55°C в стая с температура 20°C. DB/WB 7°C/6°.","(2) - Измерено при спад на налягане от 10 kPa в системата за отопление при работно състояние на изходящата вода от 47-55°C в стая с температура 20°C. DB/WB 7°C/6°."]