{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETBX16E9W / EPRA014-018DW"]
[]
[]
[]
[]
["","","","","","ETBX16EF9W / EPRA14DAW1","ETBX16EF9W / EPRA16DAW1","ETBX16EF9W / EPRA18DAW1"]
["COP","","","","","4.79","5.00 (2)","5.00"]
["Отопление с конвекция","Изходяща вода при средни климат. условия 55°C","Общо","Клас на сезонна ефективност при отопление","","","A++"]
["","","","ηs (Сезонна ефективност на отопление)","%","","142"]
["","","","SCOP","","","3.63"]
["Капацитет на охлаждане","Ном.","","","kW","","11.5 (3), 7.88 (4)"]
["EER","","","","","4.13, 2.70","4.11 (3), 2.69 (4)","4.09, 2.68"]
["Топлинен капацитет","Ном.","","","kW","","9.00 (2)"]
["","Мин.","","","kW","","3.96 (1)"]
["","Макс.","","","kW","","10.44 (1)"]
["Входяща мощност","Охлаждане","","Ном.","kW","","2.80 (3), 2.93 (4)"]
["","Отопление","","Макс.","kW","","2.32 (5)"]
["","","","Мин.","kW","","0.90 (5)"]
["","","","Ном.","kW","","1.80 (2)"]
["Забележки","","","","","(1) - Капацитет съгласно стандарт EN14511 и валиден за гамата с топла вода dT = 3~8°C при Ta 7°C","(1) - Капацитет съгласно стандарт EN14511 и валиден за гамата с топла вода dT = 3~8°C при Ta 7°C","(1) - Капацитет съгласно стандарт EN14511 и валиден за гамата с топла вода dT = 3~8°C при Ta 7°C"]
["","","","","","(2) - Условие: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Условие: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Условие: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Охлаждане: EW 23℃; LW 18℃; външни условия: 35°C по сух термометър","(3) - Охлаждане: EW 23℃; LW 18℃; външни условия: 35°C по сух термометър","(3) - Охлаждане: EW 23℃; LW 18℃; външни условия: 35°C по сух термометър"]
["","","","","","(4) - Охлаждане: EW 12℃; LW 7℃; външни условия: 35°C по сух термометър","(4) - Охлаждане: EW 12℃; LW 7℃; външни условия: 35°C по сух термометър","(4) - Охлаждане: EW 12℃; LW 7℃; външни условия: 35°C по сух термометър"]
["","","","","","(5) - Консумирана мощност е общата мощност на вътрешни и външни тела, включително и циркулационната помпа; съгласно EN14511","(5) - Консумирана мощност е общата мощност на вътрешни и външни тела, включително и циркулационната помпа; съгласно EN14511","(5) - Консумирана мощност е общата мощност на вътрешни и външни тела, включително и циркулационната помпа; съгласно EN14511"]
["","","","","","(6) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) с помпа на пълна скорост","(6) - Изпитване при Ta DB/WB 7°C/6°C. Съгласно EN 16147.","(6) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) с помпа на пълна скорост"]
["","","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) с помпа на пълна скорост"]
["Топлинен капацитет","Мин.","","","kW","3.70","","4.40"]
["","Ном.","","","kW","5.90","","9.00"]
["","Макс.","","","kW","9.75","","11.60"]
["Капацитет на охлаждане","Ном.","","","kW","10.6, 6.90","","12.5, 8.86"]
["Входяща мощност","Отопление","","Мин.","kW","0.84","","1.00"]
["","","","Ном.","kW","1.23","","1.80"]
["","","","Макс.","kW","2.17","","2.58"]
["","Охлаждане","","Ном.","kW","2.55, 2.56","","3.05, 3.31"]
["Отопление с конвекция","Изходяща вода при средни климат. условия 55°C","Общо","SCOP","","3.63","","3.63"]
["","","","Клас на сезонна ефективност при отопление","","A++","","A++"]
["","Изходяща вода при средни климат. условия 35°C","Общо","SCOP","","4.81","","4.81"]
["","","","Клас на сезонна ефективност при отопление","","A+++","","A+++"]