{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Корпус","Цвят","","","","Бяло","Бяло"]
["","Материал","","","","Смола","Смола"]
["Размери","Тяло","","Височина","mm","290","340"]
["","","","Широчина","mm","1050","1200"]
["","","","Дълбочина","mm","269","262"]
["Тегло","Тяло","","","кг","14","18"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","16.2","23"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","13.4","21.1"]
["","","","Ниско","м³/мин","12.1","18.7"]
["","","Отопление","Висок","м³/мин","16.9","23"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","14.2","20.9"]
["","","Отопление","Ниско","м³/мин","12.7","18.7"]
["Звукова мощност","Охлаждане","","","дБА","61","65"]
["","Отопление","","","дБА","61","65"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","45","49"]
["","","","Среден","дБА","42","45"]
["","","","Ниско","дБА","40","41"]
["","Отопление","","Висок","дБА","45","49"]
["","","","Среден","дБА","42","45"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","40","41"]
["Тръбни съединения","Tечност","","Вън. д.","mm","9.52","9.52"]
["","Газ","","Вън. д.","mm","15.9","15.9"]
["","Дренаж","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Електрозахранване","Фаза","","","","1~","1~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","220-240","220-240"]
["Стандартни аксесоари","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Забележки","","","","","(1) - Номиналният капацитет на охлаждане се базира на: вътрешна темп.: 27°CDB, 19°CWB, външна температура: 35°CDB, еквивалентна дължина на тръбите за хладилен агент: 5 m, разлика в нивото: 0m."]
["","","","","","(2) - Номиналният капацитет за загряване важи за: вътрешна температура: 20°C (сух термометър), външна температура: 7°C (сух термометър), 8°C (влажен термометър), съответна дължина на тръбите: 5 м, денивелация: 0m."]
["Стандартни аксесоари","Screw cover","","","","","3"]