{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9","FAQ100CVEB9"]
["Ниво на звуково налягане","Отопление","Висок","dBA","45","49"]
["","","Ном.","dBA","42","45"]
["","","Среден","dBA","42","45"]
["","","Ниско","dBA","40","41"]
["","Охлаждане","Среден","dBA","42","45"]
["","","Ниско","dBA","40","41"]
["","","Висок","dBA","45","49"]
["","","Ном.","dBA","42","45"]
["Капацитет на охлаждане","Общ капацитет","Ном.","кВт","0.051","0.061"]
["Тръбни съединения","Tечност","Вън. д.","мм","9.52","9.52"]
["","Газ","Вън. д.","мм","15.9","15.9"]
["","Дренаж","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Ниво на звукова мощност","Охлаждане","","dBA","61","65"]
["","Отопление","","dBA","61","65"]
["Размери","Тяло","Широчина","мм","1,050","1,200"]
["","","Дълбочина","мм","238","240"]
["","","Височина","мм","290","340"]
["Корпус","Материал","","","Смола","Смола"]
["","Цвят","","","Свежо бяло","Свежо бяло"]
["Тегло","Тяло","","kg","13","17"]
["Топлинен капацитет","Общ капацитет","Ном.","кВт","0.068","0.061"]
["Power supply","Фаза","","","1~","1~"]
["","Честота","","Хц","50","50"]
["","Напрежение","","V","220-240","220-240"]