{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / 3MXM-A"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / FBA35A2VEB9 / 3MXM68A2V1B"]
["Капацитет на охлаждане","Ном.","","kW","6.80"]
["Номинална ефективност","Годишен разход на енергия","","kWh","1,245"]
["","EER","","","2.73"]
["","COP","","","3.24"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","D"]
["","","Отопление","","C"]
["Топлинен капацитет","Ном.","","kW","8.60"]
["Забележки","","","","(1) - Номиналният капацитет на охлаждане се базира на: вътрешна температура: 27°CDB, 19°CWB, външна температура: 35°CDB, еквивалентна дължина на тръбите за хладилен агент: 5 m, разлика в нивото: 0m."]
["","","","","(2) - Номиналният капацитет за загряване важи за: вътрешна температура: 20°C (сух термометър), външна температура: 7°C (сух термометър), 8°C (влажен термометър), съответна дължина на тръбите: 5 м, денивелация: 0m."]
["","","","","(3) - Вж. отделния чертеж за работен диапазон"]
["","","","","(4) - Вж. отделния чертеж за електрическите схеми"]