{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / ARXM-R"]
[]
[]
[]
[]
["","","","","FBA71A2VEB9 / ARXM71R2V1B","FBA71A2VEB9 / ARXM71R5V1B"]
["Капацитет на охлаждане","Ном.","","kW","6.80","6.80"]
["","Макс.","","kW","6.98","6.98"]
["Топлинен капацитет","Ном.","","kW","7.50","7.50"]
["","Макс.","","kW","7.66","7.66"]
["Номинална ефективност","EER","","","3.60","3.60"]
["","COP","","","3.67","3.67"]
["","Годишен разход на енергия","","kWh","944","944"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A","A"]
["","","Отопление","","A","A"]
["Охлаждане с конвекция","Клас на енергийна ефективност","","","A","A"]
["","Капацитет","Pdesign","kW","6.80","6.80"]
["","SEER","","","5.57","5.57"]
["","Годишно потребление на електроенергия","","kWh/a","427","427"]
["Отопление с конвекция (умерен климат)","Клас на енергийна ефективност","","","A","A"]
["","Капацитет","Pdesign","kW","4.50","4.50"]
["","SCOP/A","","","3.81","3.81"]
["","Pdh Капацитет на отопление при -10°","","kW","4.50","4.50"]
["","Годишно потребление на електроенергия","","kWh/a","1652","1652"]
["Диапазон на енергийна ефективност","","","","A+++ ~ D","A+++ ~ D"]